# Static Call Graph for image .\obj\Project.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Sat Sep 06 10:52:01 2025

### Maximum Stack Usage = 520 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ AES_Test ⇒ AES_Func_Test ⇒ WIZAES_EncDec ⇒ MHAES_EncDec

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - ADC3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - BusFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_RX1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_SCE_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DebugMon_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI0_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI15_10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI9_5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - FLASH_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - FSMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - HardFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - MemManage_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - NMI_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - PVD_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - PendSV_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - RCC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RNG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTCAlarm_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - Reset_Handler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SDIO_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SENSOR_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SVC_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SYMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SysTick_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SystemInit from system_w55mh32.o(.text) referenced from startup_w55mh32.o(.text)
  - TAMPER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM2_IRQHandler from debug.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USBWakeUp_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UsageFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - WWDG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_w55mh32.o(.text)
  - fputc from main.o(.text) referenced from printf8.o(i.__0printf$8)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_w55mh32.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  UART_Configuration (Thumb, 112 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = UART_Configuration ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  main (Thumb, 192 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 520
  - Call Chain = main ⇒ AES_Test ⇒ AES_Func_Test ⇒ WIZAES_EncDec ⇒ MHAES_EncDec
  [Calls]
  - >> wiz_crypt_version
  - >> WIZRAND_Init
  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> AES_Test
  - >> UART_Configuration
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NVIC_Configuration (Thumb, 2 bytes, Stack size 0 bytes, main.o(.text), UNUSED)

  SER_PutChar (Thumb, 30 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SER_PutChar ⇒ USART_SendData
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> fputc

  fputc (Thumb, 24 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = fputc ⇒ SER_PutChar ⇒ USART_SendData
  [Calls]
  - >> SER_PutChar
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  printf_monobit (Thumb, 66 bytes, Stack size 24 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  printf_byte_bit (Thumb, 62 bytes, Stack size 24 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  printf_byte_bit_runs (Thumb, 74 bytes, Stack size 16 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  printf_long_runs_max (Thumb, 76 bytes, Stack size 24 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  assert_failed (Thumb, 4 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> get_time
  - >> time_add
  - >> time_avg
  - >> USART_ClearITPendingBit
  - >> USART_GetITStatus
  - >> USART_ClearFlag
  - >> USART_IrDACmd
  - >> USART_IrDAConfig
  - >> USART_OneBitMethodCmd
  - >> USART_OverSampling8Cmd
  - >> USART_HalfDuplexCmd
  - >> USART_SmartCardNACKCmd
  - >> USART_SmartCardCmd
  - >> USART_SetPrescaler
  - >> USART_SetGuardTime
  - >> USART_SendBreak
  - >> USART_ReceiveData
  - >> USART_LINCmd
  - >> USART_LINBreakDetectLengthConfig
  - >> USART_ReceiverWakeUpCmd
  - >> USART_WakeUpConfig
  - >> USART_SetAddress
  - >> USART_DMACmd
  - >> USART_ITConfig
  - >> USART_ClockInit
  - >> USART_DeInit
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> TIM_ClearFlag
  - >> TIM_GetFlagStatus
  - >> TIM_GetPrescaler
  - >> TIM_GetCounter
  - >> TIM_GetCapture4
  - >> TIM_GetCapture3
  - >> TIM_GetCapture2
  - >> TIM_GetCapture1
  - >> TIM_SetClockDivision
  - >> TIM_SetCompare4
  - >> TIM_SetCompare3
  - >> TIM_SetCompare2
  - >> TIM_SetCompare1
  - >> TIM_SetAutoreload
  - >> TIM_SetCounter
  - >> TIM_SelectMasterSlaveMode
  - >> TIM_SelectSlaveMode
  - >> TIM_SelectOutputTrigger
  - >> TIM_SelectOnePulseMode
  - >> TIM_SelectHallSensor
  - >> TIM_UpdateRequestConfig
  - >> TIM_UpdateDisableConfig
  - >> TIM_SelectOCxM
  - >> TIM_CCxNCmd
  - >> TIM_CCxCmd
  - >> TIM_OC4PolarityConfig
  - >> TIM_OC3NPolarityConfig
  - >> TIM_OC3PolarityConfig
  - >> TIM_OC2NPolarityConfig
  - >> TIM_OC2PolarityConfig
  - >> TIM_OC1NPolarityConfig
  - >> TIM_OC1PolarityConfig
  - >> TIM_ClearOC4Ref
  - >> TIM_ClearOC3Ref
  - >> TIM_ClearOC2Ref
  - >> TIM_ClearOC1Ref
  - >> TIM_OC4FastConfig
  - >> TIM_OC3FastConfig
  - >> TIM_OC2FastConfig
  - >> TIM_OC1FastConfig
  - >> TIM_OC4PreloadConfig
  - >> TIM_OC3PreloadConfig
  - >> TIM_OC2PreloadConfig
  - >> TIM_OC1PreloadConfig
  - >> TIM_CCPreloadControl
  - >> TIM_SelectCCDMA
  - >> TIM_SelectCOM
  - >> TIM_ARRPreloadConfig
  - >> TIM_ForcedOC4Config
  - >> TIM_ForcedOC3Config
  - >> TIM_ForcedOC2Config
  - >> TIM_ForcedOC1Config
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_CounterModeConfig
  - >> TIM_PrescalerConfig
  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config
  - >> TIM_ETRConfig
  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig
  - >> TIM_SelectInputTrigger
  - >> TIM_InternalClockConfig
  - >> TIM_DMACmd
  - >> TIM_DMAConfig
  - >> TIM_GenerateEvent
  - >> TIM_ITConfig
  - >> TIM_CtrlPWMOutputs
  - >> TIM_Cmd
  - >> TIM_BDTRConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit
  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TIM_OC4Init
  - >> TIM_OC3Init
  - >> TIM_OC2Init
  - >> TIM_OC1Init
  - >> TIM_TimeBaseInit
  - >> TIM_DeInit
  - >> RCC_ClearITPendingBit
  - >> RCC_GetITStatus
  - >> RCC_MCOConfig
  - >> RCC_ClockSecuritySystemCmd
  - >> RCC_BackupResetCmd
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  - >> RCC_RTCCLKCmd
  - >> RCC_RTCCLKConfig
  - >> RCC_LSICmd
  - >> RCC_LSEConfig
  - >> RCC_ADCCLKConfig
  - >> RCC_USBCLKConfig
  - >> RCC_ITConfig
  - >> RCC_HSICmd
  - >> RCC_AdjustHSICalibrationValue
  - >> RCC_APB2PeriphResetCmd
  - >> GPIO_ForceDropDownConfig
  - >> GPIO_ForcePullUpConfig
  - >> GPIO_ForcePuPdCmd
  - >> GPIO_ETH_MediaInterfaceConfig
  - >> GPIO_EXTILineConfig
  - >> GPIO_PinRemapConfigUser
  - >> GPIO_PinRemapConfig
  - >> GPIO_EventOutputCmd
  - >> GPIO_EventOutputConfig
  - >> GPIO_PinLockConfig
  - >> GPIO_Write
  - >> GPIO_WriteBit
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadOutputData
  - >> GPIO_ReadOutputDataBit
  - >> GPIO_ReadInputData
  - >> GPIO_ReadInputDataBit
  - >> GPIO_DeInit
  - >> SysTick_CLKSourceConfig
  - >> NVIC_SystemLPConfig
  - >> NVIC_SetVectorTable
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  - >> USART_SendData
  - >> USART_Init
  - >> USART_GetFlagStatus
  - >> USART_Cmd
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetFlagStatus
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  BOOT_RAM (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SENSOR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SYMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 48 bytes, Stack size 8 bytes, misc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  NVIC_Init (Thumb, 158 bytes, Stack size 24 bytes, misc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> timer_init_ms

  NVIC_SetVectorTable (Thumb, 60 bytes, Stack size 16 bytes, misc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  NVIC_SystemLPConfig (Thumb, 78 bytes, Stack size 16 bytes, misc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  SysTick_CLKSourceConfig (Thumb, 62 bytes, Stack size 8 bytes, misc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_DeInit (Thumb, 224 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> assert_failed

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 378 bytes, Stack size 40 bytes, w55mh32_gpio.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = GPIO_Init
  [Calls]
  - >> assert_failed
  [Called By]
  - >> UART_Configuration

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 170 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ReadInputData (Thumb, 64 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ReadOutputDataBit (Thumb, 252 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ReadOutputData (Thumb, 66 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_SetBits (Thumb, 86 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ResetBits (Thumb, 86 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_WriteBit (Thumb, 188 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_Write (Thumb, 66 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_PinLockConfig (Thumb, 100 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_EventOutputConfig (Thumb, 138 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_EventOutputCmd (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_PinRemapConfig (Thumb, 552 bytes, Stack size 32 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_PinRemapConfigUser (Thumb, 102 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_EXTILineConfig (Thumb, 186 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ETH_MediaInterfaceConfig (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ForcePuPdCmd (Thumb, 100 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ForcePullUpConfig (Thumb, 164 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  GPIO_ForceDropDownConfig (Thumb, 170 bytes, Stack size 16 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> main

  RCC_HSEConfig (Thumb, 98 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_HSEConfig
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_GetFlagStatus (Thumb, 118 bytes, Stack size 24 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_GetFlagStatus
  [Calls]
  - >> assert_failed
  [Called By]
  - >> RCC_WaitForHSEStartUp
  - >> main

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = RCC_WaitForHSEStartUp ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> main

  RCC_AdjustHSICalibrationValue (Thumb, 36 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_HSICmd (Thumb, 28 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_PLLConfig (Thumb, 250 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_PLLConfig
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_PLLCmd (Thumb, 28 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_PLLCmd
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_SYSCLKConfig (Thumb, 42 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_SYSCLKConfig
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 66 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_HCLKConfig
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_PCLK1Config (Thumb, 58 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_PCLK1Config
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_PCLK2Config (Thumb, 60 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_PCLK2Config
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main

  RCC_ITConfig (Thumb, 70 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_USBCLKConfig (Thumb, 212 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_ADCCLKConfig (Thumb, 130 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_LSEConfig (Thumb, 78 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_LSICmd (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_RTCCLKConfig (Thumb, 48 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_RTCCLKCmd (Thumb, 32 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_GetClocksFreq (Thumb, 228 bytes, Stack size 20 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 78 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_APB2PeriphClockCmd (Thumb, 74 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_APB2PeriphClockCmd
  [Calls]
  - >> assert_failed
  [Called By]
  - >> main
  - >> UART_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 74 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> timer_config

  RCC_APB2PeriphResetCmd (Thumb, 74 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> USART_DeInit
  - >> TIM_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 74 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> USART_DeInit
  - >> TIM_DeInit

  RCC_BackupResetCmd (Thumb, 104 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_ClockSecuritySystemCmd (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_MCOConfig (Thumb, 116 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 62 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  RCC_ClearITPendingBit (Thumb, 32 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_DeInit (Thumb, 440 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  - >> assert_failed
  [Called By]
  - >> timer_config

  TIM_TimeBaseInit (Thumb, 272 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> timer_config

  TIM_OC1Init (Thumb, 498 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC2Init (Thumb, 432 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC3Init (Thumb, 416 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC4Init (Thumb, 332 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetIC4Prescaler (Thumb, 110 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 102 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 122 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 138 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 576 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config
  - >> assert_failed

  TIM_PWMIConfig (Thumb, 186 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> assert_failed

  TIM_BDTRConfig (Thumb, 236 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 202 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> get_time
  - >> timer_init_ms

  TIM_CtrlPWMOutputs (Thumb, 82 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ITConfig (Thumb, 166 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> timer_init_ms

  TIM_GenerateEvent (Thumb, 130 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_DMAConfig (Thumb, 270 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_DMACmd (Thumb, 126 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_InternalClockConfig (Thumb, 76 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectInputTrigger (Thumb, 184 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 110 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> assert_failed

  TIM_TIxExternalClockConfig (Thumb, 180 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config
  - >> assert_failed

  TIM_ETRConfig (Thumb, 164 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed
  [Called By]
  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 172 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig
  - >> assert_failed

  TIM_ETRClockMode2Config (Thumb, 152 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig
  - >> assert_failed

  TIM_PrescalerConfig (Thumb, 128 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_CounterModeConfig (Thumb, 156 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_EncoderInterfaceConfig (Thumb, 206 bytes, Stack size 32 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ForcedOC1Config (Thumb, 126 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ForcedOC2Config (Thumb, 110 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ForcedOC3Config (Thumb, 90 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ForcedOC4Config (Thumb, 98 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ARRPreloadConfig (Thumb, 144 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectCOM (Thumb, 72 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectCCDMA (Thumb, 96 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_CCPreloadControl (Thumb, 154 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC1PreloadConfig (Thumb, 124 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC2PreloadConfig (Thumb, 108 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC3PreloadConfig (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC4PreloadConfig (Thumb, 96 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC1FastConfig (Thumb, 124 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC2FastConfig (Thumb, 108 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC3FastConfig (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC4FastConfig (Thumb, 96 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ClearOC1Ref (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ClearOC2Ref (Thumb, 144 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ClearOC3Ref (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ClearOC4Ref (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC1PolarityConfig (Thumb, 124 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC1NPolarityConfig (Thumb, 64 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC2PolarityConfig (Thumb, 108 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC2NPolarityConfig (Thumb, 72 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC3PolarityConfig (Thumb, 96 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC3NPolarityConfig (Thumb, 72 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_OC4PolarityConfig (Thumb, 96 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_CCxCmd (Thumb, 218 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_CCxNCmd (Thumb, 104 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectOCxM (Thumb, 246 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_UpdateDisableConfig (Thumb, 144 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_UpdateRequestConfig (Thumb, 144 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectHallSensor (Thumb, 108 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectOnePulseMode (Thumb, 138 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectOutputTrigger (Thumb, 196 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectSlaveMode (Thumb, 112 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SelectMasterSlaveMode (Thumb, 102 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetCounter (Thumb, 106 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetAutoreload (Thumb, 106 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetCompare1 (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetCompare2 (Thumb, 70 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetCompare3 (Thumb, 58 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetCompare4 (Thumb, 60 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_SetClockDivision (Thumb, 134 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetCapture1 (Thumb, 92 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetCapture2 (Thumb, 126 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetCapture3 (Thumb, 56 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetCapture4 (Thumb, 58 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetCounter (Thumb, 104 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetPrescaler (Thumb, 104 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetFlagStatus (Thumb, 188 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_ClearFlag (Thumb, 128 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  TIM_GetITStatus (Thumb, 186 bytes, Stack size 24 bytes, w55mh32_tim.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = TIM_GetITStatus
  [Calls]
  - >> assert_failed
  [Called By]
  - >> TIM2_IRQHandler

  TIM_ClearITPendingBit (Thumb, 128 bytes, Stack size 16 bytes, w55mh32_tim.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_ClearITPendingBit
  [Calls]
  - >> assert_failed
  [Called By]
  - >> TIM2_IRQHandler
  - >> timer_init_ms

  USART_DeInit (Thumb, 174 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  - >> assert_failed

  USART_Init (Thumb, 470 bytes, Stack size 56 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  - >> assert_failed
  [Called By]
  - >> UART_Configuration

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 162 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 90 bytes, Stack size 16 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_Cmd
  [Calls]
  - >> assert_failed
  [Called By]
  - >> UART_Configuration

  USART_ITConfig (Thumb, 332 bytes, Stack size 32 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_DMACmd (Thumb, 114 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SetAddress (Thumb, 86 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_WakeUpConfig (Thumb, 90 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_ReceiverWakeUpCmd (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_LINBreakDetectLengthConfig (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_LINCmd (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SendData (Thumb, 78 bytes, Stack size 16 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_SendData
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SER_PutChar

  USART_ReceiveData (Thumb, 56 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SendBreak (Thumb, 58 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SetGuardTime (Thumb, 54 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SetPrescaler (Thumb, 66 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SmartCardCmd (Thumb, 102 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_SmartCardNACKCmd (Thumb, 82 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_HalfDuplexCmd (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_OverSampling8Cmd (Thumb, 92 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_OneBitMethodCmd (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_IrDAConfig (Thumb, 88 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_IrDACmd (Thumb, 94 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_GetFlagStatus (Thumb, 164 bytes, Stack size 16 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetFlagStatus
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SER_PutChar

  USART_ClearFlag (Thumb, 122 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_GetITStatus (Thumb, 280 bytes, Stack size 32 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  USART_ClearITPendingBit (Thumb, 158 bytes, Stack size 24 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_w55mh32.o(.text)

  SystemCoreClockUpdate (Thumb, 160 bytes, Stack size 8 bytes, system_w55mh32.o(.text), UNUSED)

  r_printf (Thumb, 44 bytes, Stack size 16 bytes, debug.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = r_printf ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> AES_Func_Test

  ouputRes (Thumb, 50 bytes, Stack size 24 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  ouputArrayHex (Thumb, 50 bytes, Stack size 24 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  timer_config (Thumb, 66 bytes, Stack size 24 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> TIM_TimeBaseInit
  - >> TIM_DeInit
  - >> RCC_APB1PeriphClockCmd
  [Called By]
  - >> timer_init_ms

  timer_init_ms (Thumb, 70 bytes, Stack size 16 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> timer_config
  - >> TIM_ClearITPendingBit
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> NVIC_Init

  time_avg (Thumb, 84 bytes, Stack size 16 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  time_add (Thumb, 90 bytes, Stack size 16 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> assert_failed

  get_time (Thumb, 44 bytes, Stack size 16 bytes, debug.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd
  - >> assert_failed

  timer_Verify (Thumb, 2 bytes, Stack size 0 bytes, debug.o(.text), UNUSED)

  TIM2_IRQHandler (Thumb, 32 bytes, Stack size 8 bytes, debug.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM2_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  AES_Func_Test (Thumb, 416 bytes, Stack size 400 bytes, aes_self_test.o(.text))
  [Stack]

  - Max Depth = 504
  - Call Chain = AES_Func_Test ⇒ WIZAES_EncDec ⇒ MHAES_EncDec
  [Calls]
  - >> WIZCRC_CalcBuff
  - >> WIZAES_EncDec
  - >> r_printf
  - >> memcmp
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  [Called By]
  - >> AES_Test

  AES_Test (Thumb, 8 bytes, Stack size 8 bytes, aes_self_test.o(.text))
  [Stack]

  - Max Depth = 512
  - Call Chain = AES_Test ⇒ AES_Func_Test ⇒ WIZAES_EncDec ⇒ MHAES_EncDec
  [Calls]
  - >> AES_Func_Test
  [Called By]
  - >> main

  mh_crypt_version (Thumb, 4 bytes, Stack size 0 bytes, mh_crypt_version.o(.text))
  [Called By]

  - >> wiz_crypt_version

  mh_crypt_date (Thumb, 4 bytes, Stack size 0 bytes, mh_crypt_version.o(.text), UNUSED)

  mh_crypt_time (Thumb, 4 bytes, Stack size 0 bytes, mh_crypt_version.o(.text), UNUSED)

  MHAES_EncDec (Thumb, 740 bytes, Stack size 88 bytes, mh_aes.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = MHAES_EncDec
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> MHSYMC_FuncEnable
  [Called By]
  - >> WIZAES_EncDec

  MHRAND_Init (Thumb, 208 bytes, Stack size 32 bytes, mh_rand.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MHRAND_Init
  [Calls]
  - >> __aeabi_memclr4
  - >> NVIC_DisableIRQ
  - >> NVIC_EnableIRQ
  [Called By]
  - >> WIZRAND_Init

  MHCRC_CalcBuff (Thumb, 52 bytes, Stack size 24 bytes, mh_rand.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = MHCRC_CalcBuff
  [Called By]
  - >> WIZCRC_CalcBuff
  - >> MHRAND_UpdatePSeed
  - >> MHRAND_TrandNoBlk
  - >> MHRAND_Trand

  MHRAND_Prand (Thumb, 104 bytes, Stack size 16 bytes, mh_rand.o(.text), UNUSED)
  [Called By]

  - >> MHRAND_Trand

  MHRAND_TrandNoBlk (Thumb, 292 bytes, Stack size 72 bytes, mh_rand.o(.text), UNUSED)
  [Calls]

  - >> MHRAND_GetRandWord
  - >> MHCRC_CalcBuff
  [Called By]
  - >> MHRAND_Trand

  MHRAND_Trand (Thumb, 178 bytes, Stack size 56 bytes, mh_rand.o(.text), UNUSED)
  [Calls]

  - >> MHCRC_CalcBuff
  - >> MHRAND_Prand
  - >> MHRAND_TrandNoBlk
  [Called By]
  - >> MHRAND_UpdatePSeed

  MHRAND_UpdatePSeed (Thumb, 70 bytes, Stack size 24 bytes, mh_rand.o(.text), UNUSED)
  [Calls]

  - >> MHCRC_CalcBuff
  - >> MHRAND_Trand

  TRNG_IRQHandler (Thumb, 220 bytes, Stack size 32 bytes, mh_rand.o(.text), UNUSED)
  [Calls]

  - >> NVIC_DisableIRQ
  - >> MHCRC_CalcWord

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> MHAES_EncDec

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> AES_Func_Test

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> MHRAND_GetRandWord

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> AES_Func_Test
  - >> MHRAND_Init
  - >> MHAES_EncDec

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> AES_Func_Test

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  WIZAES_EncDec (Thumb, 16 bytes, Stack size 16 bytes, wiz_crypt.o(.text.WIZAES_EncDec))
  [Stack]

  - Max Depth = 104
  - Call Chain = WIZAES_EncDec ⇒ MHAES_EncDec
  [Calls]
  - >> MHAES_EncDec
  [Called By]
  - >> AES_Func_Test

  WIZCRC_CalcBuff (Thumb, 28 bytes, Stack size 24 bytes, wiz_crypt.o(.text.WIZCRC_CalcBuff))
  [Stack]

  - Max Depth = 48
  - Call Chain = WIZCRC_CalcBuff ⇒ MHCRC_CalcBuff
  [Calls]
  - >> MHCRC_CalcBuff
  [Called By]
  - >> AES_Func_Test

  WIZRAND_Init (Thumb, 20 bytes, Stack size 16 bytes, wiz_crypt.o(.text.WIZRAND_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = WIZRAND_Init ⇒ MHRAND_Init
  [Calls]
  - >> MHRAND_Init
  [Called By]
  - >> main

  wiz_crypt_version (Thumb, 8 bytes, Stack size 8 bytes, wiz_crypt.o(.text.wiz_crypt_version))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiz_crypt_version
  [Calls]
  - >> mh_crypt_version
  [Called By]
  - >> main

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> ouputArrayHex
  - >> ouputRes
  - >> r_printf
  - >> printf_long_runs_max
  - >> printf_byte_bit_runs
  - >> printf_byte_bit
  - >> printf_monobit
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 154 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  MHSYMC_FuncEnable (Thumb, 26 bytes, Stack size 0 bytes, mh_aes.o(.text))
  [Called By]

  - >> MHAES_EncDec

  MHCRC_CalcWord (Thumb, 48 bytes, Stack size 28 bytes, mh_rand.o(.text), UNUSED)
  [Called By]

  - >> TRNG_IRQHandler
  - >> MHRAND_GetRandWord

  MHRAND_GetRandWord (Thumb, 218 bytes, Stack size 8 bytes, mh_rand.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr
  - >> NVIC_DisableIRQ
  - >> NVIC_EnableIRQ
  - >> MHCRC_CalcWord
  [Called By]
  - >> MHRAND_TrandNoBlk

  NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, mh_rand.o(.text))
  [Called By]

  - >> MHRAND_GetRandWord
  - >> MHRAND_Init

  NVIC_DisableIRQ (Thumb, 18 bytes, Stack size 0 bytes, mh_rand.o(.text))
  [Called By]

  - >> TRNG_IRQHandler
  - >> MHRAND_GetRandWord
  - >> MHRAND_Init

  _printf_core (Thumb, 984 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols