# Static Call Graph for image ..\Output\Project.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Apr 22 13:15:42 2026

### Maximum Stack Usage = 1664 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ start_iperf_test ⇒ exchange_results ⇒ cJSON_PrintUnformatted ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- cJSON_Delete ⇒ cJSON_Delete
- print_array ⇒ print_value
- print_object ⇒ print_value
- parse_array ⇒ parse_value
- parse_object ⇒ parse_value

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - ADC3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - BusFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_RX1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_SCE_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel4_IRQHandler from w55mh32_wztoe.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel5_IRQHandler from w55mh32_wztoe.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DebugMon_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI0_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI15_10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI9_5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - FLASH_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - FSMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - HardFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - MemManage_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - NMI_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - PVD_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - PendSV_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - RCC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RNG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTCAlarm_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - Reset_Handler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SDIO_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SENSOR_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SVC_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SYMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SysTick_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SystemInit from system_w55mh32.o(.text) referenced from startup_w55mh32.o(.text)
  - TAMPER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM3_IRQHandler from bsp_tim.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USBWakeUp_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UsageFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - WWDG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_w55mh32.o(.text)
  - _sbackspace from _sgetc.o(.text) referenced 2 times from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced 2 times from __0sscanf.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - default_ip_assign from dhcp.o(.text) referenced from dhcp.o(.data)
  - default_ip_assign from dhcp.o(.text) referenced from dhcp.o(.text)
  - default_ip_conflict from dhcp.o(.text) referenced from dhcp.o(.data)
  - default_ip_conflict from dhcp.o(.text) referenced from dhcp.o(.text)
  - default_ip_update from dhcp.o(.text) referenced from dhcp.o(.data)
  - default_ip_update from dhcp.o(.text) referenced from dhcp.o(.text)
  - fputc from bsp_uart.o(.text) referenced from printfa.o(i.__0printf)
  - free from mallocr.o(i.__free$realloc) referenced from cjson.o(.data)
  - free from mallocr.o(i.__free$realloc) referenced from cjson.o(.text)
  - isspace from isspace_c.o(.text) referenced 2 times from scanf_char.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - malloc from mallocr.o(i.__malloc$realloc) referenced from cjson.o(.data)
  - malloc from mallocr.o(i.__malloc$realloc) referenced from cjson.o(.text)
  - realloc from mallocr.o(i.realloc) referenced from cjson.o(.data)
  - realloc from mallocr.o(i.realloc) referenced from cjson.o(.text)
  - wiz_deselect from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wiz_read_buff from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wiz_read_byte from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wiz_select from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wiz_write_buff from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wiz_write_byte from w55mh32_wztoe.o(.text) referenced from w55mh32_wztoe.o(.text)
  - wizchip_bus_readdata from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_bus_writedata from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_cris_enter from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_cris_enter from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cris_exit from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_cris_exit from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cs_deselect from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_cs_deselect from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cs_select from wizchip_conf.o(.text) referenced from wizchip_conf.o(.data)
  - wizchip_cs_select from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_readburst from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_readbyte from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_writeburst from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_writebyte from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_w55mh32.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  BOOT_RAM (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SENSOR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SYMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> tim3_init
  - >> spi_dma_init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> rcc_clk_config
  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 230 bytes, Stack size 20 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> tim3_init
  - >> delay_init
  - >> I2S_Init
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> spi_dma_init

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> console_usart_init
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> tim3_init
  - >> wiztoe_bus_init

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, w55mh32_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> console_usart_init
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text))
  [Called By]

  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init
  - >> wiz_deselect

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text))
  [Called By]

  - >> wiztoe_hw_reset
  - >> wiz_select

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfigUser (Thumb, 50 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForcePuPdCmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForcePullUpConfig (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForceDropDownConfig (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 230 bytes, Stack size 56 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> console_usart_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> console_usart_init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 104 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, w55mh32_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, w55mh32_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> wiztoe_bus_init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, w55mh32_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiztoe_bus_init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiz_read_byte
  - >> wiz_write_byte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiz_read_byte
  - >> wiz_write_byte
  - >> spi_dma_transfer

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiz_deselect
  - >> wiz_select
  - >> wiz_read_byte
  - >> wiz_write_byte
  - >> spi_dma_transfer

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiztoe_bus_init

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_spi.o(.text), UNUSED)

  TIM_DeInit (Thumb, 346 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 104 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_OC1Init (Thumb, 114 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 150 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 114 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 78 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 150 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 32 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 82 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, w55mh32_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM3_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  DMA1_Channel4_IRQHandler (Thumb, 52 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA1_Channel4_IRQHandler
  [Calls]
  - >> DMA_GetITStatus
  - >> DMA_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA1_Channel5_IRQHandler
  [Calls]
  - >> DMA_GetITStatus
  - >> DMA_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  WIZCHIP_READ (Thumb, 112 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = WIZCHIP_READ
  [Called By]
  - >> ctlwizchip
  - >> DHCP_run
  - >> wiz_print_phy_info
  - >> socket
  - >> listen
  - >> handle_create_streams
  - >> disconnect
  - >> close
  - >> main
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> wiz_send_data
  - >> getSn_RX_RSR
  - >> getSn_TX_FSR
  - >> wiz_toe_init
  - >> check_DHCP_leasedIP
  - >> default_ip_conflict
  - >> default_ip_update
  - >> wizphy_getphystat
  - >> wizchip_setnetmode
  - >> wizchip_getnetmode
  - >> wizchip_gettimeout
  - >> wizchip_sw_reset
  - >> wizchip_getinterrupt
  - >> wizchip_getinterruptmask
  - >> wizphy_getphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> wizphy_getphypmode
  - >> wizphy_getphylink
  - >> setsockopt
  - >> ctlsocket
  - >> connect
  - >> sendto
  - >> send
  - >> recvfrom
  - >> recv
  - >> getsockopt

  WIZCHIP_WRITE_BUF (Thumb, 132 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = WIZCHIP_WRITE_BUF
  [Called By]
  - >> wizchip_setnetinfo
  - >> DHCP_init
  - >> wiz_send_data
  - >> wiz_toe_init
  - >> default_ip_conflict
  - >> default_ip_update
  - >> default_ip_assign
  - >> wizchip_sw_reset
  - >> setsockopt
  - >> connect
  - >> sendto

  wiz_toe_init (Thumb, 138 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = wiz_toe_init ⇒ wiztoe_bus_init ⇒ spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> reg_wizchip_spiburst_cbfunc
  - >> reg_wizchip_spi_cbfunc
  - >> reg_wizchip_cs_cbfunc
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init
  - >> wiztoe_delay
  [Called By]
  - >> main

  WIZCHIP_WRITE (Thumb, 112 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip
  - >> wizchip_init
  - >> socket
  - >> listen
  - >> disconnect
  - >> close
  - >> main
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> wiz_send_data
  - >> check_DHCP_leasedIP
  - >> default_ip_conflict
  - >> default_ip_update
  - >> wizchip_setnetmode
  - >> wizchip_settimeout
  - >> wizchip_sw_reset
  - >> wizchip_clrinterrupt
  - >> wizchip_setinterruptmask
  - >> wizphy_setphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> setsockopt
  - >> ctlsocket
  - >> connect
  - >> sendto
  - >> send
  - >> recvfrom
  - >> recv

  WIZCHIP_READ_BUF (Thumb, 136 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = WIZCHIP_READ_BUF
  [Called By]
  - >> DHCP_init
  - >> wiz_dhcp_process
  - >> wizchip_getnetinfo
  - >> socket
  - >> main
  - >> wiz_recv_data
  - >> makeDHCPMSG
  - >> wizchip_sw_reset
  - >> getsockopt

  getSn_TX_FSR (Thumb, 108 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = getSn_TX_FSR ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> sendto
  - >> send
  - >> recv
  - >> getsockopt

  getSn_RX_RSR (Thumb, 154 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = getSn_RX_RSR ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test
  - >> handle_create_streams
  - >> parseDHCPMSG
  - >> recvfrom
  - >> recv
  - >> getsockopt

  wiz_send_data (Thumb, 132 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> sendto
  - >> send

  wiz_recv_data (Thumb, 132 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = wiz_recv_data ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> recvfrom
  - >> recv

  wiz_recv_ignore (Thumb, 102 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wiz_recv_ignore ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> recvfrom

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> spi_dma_transfer
  - >> spi_dma_init

  DMA_Init (Thumb, 60 bytes, Stack size 8 bytes, w55mh32_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> spi_dma_transfer

  DMA_StructInit (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> spi_dma_transfer
  - >> spi_dma_init

  DMA_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> spi_dma_init

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 40 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_ClearFlag (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_GetITStatus (Thumb, 40 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel4_IRQHandler

  DMA_ClearITPendingBit (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel4_IRQHandler

  main (Thumb, 460 bytes, Stack size 88 bytes, main.o(.text))
  [Stack]

  - Max Depth = 1664
  - Call Chain = main ⇒ start_iperf_test ⇒ exchange_results ⇒ cJSON_PrintUnformatted ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> wizchip_init
  - >> wizchip_getnetinfo
  - >> wiz_phy_link_check
  - >> tim3_init
  - >> stats_init
  - >> start_iperf_test
  - >> socket
  - >> rcc_clk_config
  - >> network_init
  - >> listen
  - >> handle_param_exchange
  - >> handle_create_streams
  - >> disconnect
  - >> delay_init
  - >> console_usart_init
  - >> close
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_WRITE
  - >> wiz_toe_init
  - >> WIZCHIP_READ
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_w55mh32.o(.text)

  SystemCoreClockUpdate (Thumb, 160 bytes, Stack size 8 bytes, system_w55mh32.o(.text), UNUSED)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  wiz_print_phy_info (Thumb, 54 bytes, Stack size 8 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wiz_print_phy_info ⇒ __2printf
  [Calls]
  - >> WIZCHIP_READ
  - >> __2printf
  [Called By]
  - >> wiz_phy_link_check

  wiz_phy_link_check (Thumb, 56 bytes, Stack size 8 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = wiz_phy_link_check ⇒ ctlwizchip ⇒ wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> delay_ms
  - >> ctlwizchip
  - >> wiz_print_phy_info
  - >> __2printf
  [Called By]
  - >> main

  print_network_information (Thumb, 190 bytes, Stack size 40 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = print_network_information ⇒ wizchip_getnetinfo ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> wizchip_getnetinfo
  - >> __2printf
  [Called By]
  - >> network_init

  network_init (Thumb, 46 bytes, Stack size 16 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = network_init ⇒ wiz_dhcp_process ⇒ DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_setnetinfo
  - >> print_network_information
  - >> wiz_dhcp_process
  [Called By]
  - >> main

  tim3_init (Thumb, 112 bytes, Stack size 40 bytes, bsp_tim.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = tim3_init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_GetClocksFreq
  - >> NVIC_Init
  [Called By]
  - >> main

  get_time_ms (Thumb, 6 bytes, Stack size 0 bytes, bsp_tim.o(.text))
  [Called By]

  - >> stats_stop
  - >> stats_update
  - >> stats_start

  TIM3_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, bsp_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM3_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> DHCP_time_handler
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  console_usart_init (Thumb, 118 bytes, Stack size 32 bytes, bsp_uart.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = console_usart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Cmd
  - >> USART_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  fputc (Thumb, 32 bytes, Stack size 16 bytes, bsp_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  delay_init (Thumb, 76 bytes, Stack size 24 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = delay_init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text), UNUSED)

  delay_ms (Thumb, 126 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> wiz_phy_link_check

  rcc_clk_config (Thumb, 124 bytes, Stack size 8 bytes, bsp_rcc.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = rcc_clk_config ⇒ WIZ_RCC_PLLConfig ⇒ MH_RCC_PLLConfig
  [Calls]
  - >> RCC_LSICmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HCLKConfig
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLCmd
  - >> RCC_HSICmd
  - >> RCC_GetFlagStatus
  - >> RCC_HSEConfig
  - >> RCC_DeInit
  - >> WIZ_RCC_PLLConfig
  [Called By]
  - >> main

  cJSON_GetErrorPtr (Thumb, 12 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> handle_param_exchange

  cJSON_IsString (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_GetStringValue

  cJSON_GetStringValue (Thumb, 20 bytes, Stack size 4 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_IsString

  cJSON_IsNumber (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_GetNumberValue

  cJSON_GetNumberValue (Thumb, 24 bytes, Stack size 4 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_IsNumber

  cJSON_Version (Thumb, 22 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __2sprintf

  cJSON_InitHooks (Thumb, 82 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_Delete (Thumb, 92 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 16 + In Cycle
  - Call Chain = cJSON_Delete ⇒ cJSON_Delete (Cycle)
  [Calls]
  - >> cJSON_Delete
  [Called By]
  - >> handle_param_exchange
  - >> exchange_results
  - >> cJSON_Duplicate_rec
  - >> cJSON_CreateStringArray
  - >> cJSON_CreateDoubleArray
  - >> cJSON_CreateFloatArray
  - >> cJSON_CreateIntArray
  - >> cJSON_ReplaceItemViaPointer
  - >> cJSON_DeleteItemFromObjectCaseSensitive
  - >> cJSON_DeleteItemFromObject
  - >> cJSON_DeleteItemFromArray
  - >> cJSON_AddArrayToObject
  - >> cJSON_AddObjectToObject
  - >> cJSON_AddRawToObject
  - >> cJSON_CreateRaw
  - >> cJSON_AddStringToObject
  - >> cJSON_CreateString
  - >> cJSON_AddNumberToObject
  - >> cJSON_AddBoolToObject
  - >> cJSON_AddFalseToObject
  - >> cJSON_AddTrueToObject
  - >> cJSON_AddNullToObject
  - >> cJSON_ParseWithLengthOpts
  - >> cJSON_Delete
  - >> parse_array
  - >> parse_object

  cJSON_SetNumberHelper (Thumb, 72 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_d2iz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple

  cJSON_free (Thumb, 16 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_SetValuestring
  - >> replace_item_in_object

  cJSON_SetValuestring (Thumb, 130 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> strcpy
  - >> strlen
  - >> cJSON_free
  - >> cJSON_strdup

  cJSON_ParseWithLengthOpts (Thumb, 204 bytes, Stack size 72 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 400
  - Call Chain = cJSON_ParseWithLengthOpts ⇒ parse_value ⇒ parse_number ⇒ strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> __aeabi_memclr4
  - >> cJSON_Delete
  - >> parse_value
  - >> skip_utf8_bom
  - >> buffer_skip_whitespace
  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_ParseWithLength
  - >> cJSON_ParseWithOpts

  cJSON_ParseWithOpts (Thumb, 40 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 424
  - Call Chain = cJSON_ParseWithOpts ⇒ cJSON_ParseWithLengthOpts ⇒ parse_value ⇒ parse_number ⇒ strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> strlen
  - >> cJSON_ParseWithLengthOpts
  [Called By]
  - >> cJSON_Parse

  cJSON_Parse (Thumb, 16 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 432
  - Call Chain = cJSON_Parse ⇒ cJSON_ParseWithOpts ⇒ cJSON_ParseWithLengthOpts ⇒ parse_value ⇒ parse_number ⇒ strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> cJSON_ParseWithOpts
  [Called By]
  - >> handle_param_exchange

  cJSON_ParseWithLength (Thumb, 20 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_ParseWithLengthOpts

  cJSON_Print (Thumb, 16 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 432
  - Call Chain = cJSON_Print ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> print
  [Called By]
  - >> handle_param_exchange

  cJSON_PrintUnformatted (Thumb, 16 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 432
  - Call Chain = cJSON_PrintUnformatted ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> print
  [Called By]
  - >> exchange_results

  cJSON_PrintBuffered (Thumb, 92 bytes, Stack size 56 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> print_value

  cJSON_PrintPreallocated (Thumb, 64 bytes, Stack size 56 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> print_value

  cJSON_GetArraySize (Thumb, 28 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_GetArrayItem (Thumb, 24 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> get_array_item

  cJSON_GetObjectItem (Thumb, 18 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = cJSON_GetObjectItem ⇒ get_object_item ⇒ case_insensitive_strcmp
  [Calls]
  - >> get_object_item
  [Called By]
  - >> handle_param_exchange
  - >> cJSON_DetachItemFromObject
  - >> cJSON_HasObjectItem

  cJSON_GetObjectItemCaseSensitive (Thumb, 18 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> get_object_item
  [Called By]
  - >> cJSON_DetachItemFromObjectCaseSensitive

  cJSON_HasObjectItem (Thumb, 24 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_GetObjectItem

  cJSON_AddItemToArray (Thumb, 16 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = cJSON_AddItemToArray ⇒ add_item_to_array
  [Calls]
  - >> add_item_to_array
  [Called By]
  - >> exchange_results

  cJSON_AddItemToObject (Thumb, 26 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = cJSON_AddItemToObject ⇒ add_item_to_object ⇒ cJSON_strdup
  [Calls]
  - >> add_item_to_object
  [Called By]
  - >> exchange_results

  cJSON_AddItemToObjectCS (Thumb, 26 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> add_item_to_object

  cJSON_AddItemReferenceToArray (Thumb, 32 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> add_item_to_array
  - >> create_reference

  cJSON_AddItemReferenceToObject (Thumb, 44 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> add_item_to_object
  - >> create_reference

  cJSON_CreateNull (Thumb, 20 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_AddNullToObject

  cJSON_AddNullToObject (Thumb, 44 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateNull
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateTrue (Thumb, 20 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_AddTrueToObject

  cJSON_AddTrueToObject (Thumb, 44 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateTrue
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateFalse (Thumb, 20 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_AddFalseToObject

  cJSON_AddFalseToObject (Thumb, 50 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateFalse
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateBool (Thumb, 28 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_AddBoolToObject

  cJSON_AddBoolToObject (Thumb, 48 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateBool
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateNumber (Thumb, 82 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = cJSON_CreateNumber ⇒ __aeabi_d2iz
  [Calls]
  - >> __aeabi_d2iz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_CreateDoubleArray
  - >> cJSON_CreateFloatArray
  - >> cJSON_CreateIntArray
  - >> cJSON_AddNumberToObject

  cJSON_AddNumberToObject (Thumb, 56 bytes, Stack size 32 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = cJSON_AddNumberToObject ⇒ add_item_to_object ⇒ cJSON_strdup
  [Calls]
  - >> cJSON_CreateNumber
  - >> cJSON_Delete
  - >> add_item_to_object
  [Called By]
  - >> exchange_results

  cJSON_CreateString (Thumb, 46 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = cJSON_CreateString ⇒ cJSON_strdup
  [Calls]
  - >> cJSON_Delete
  - >> cJSON_New_Item
  - >> cJSON_strdup
  [Called By]
  - >> cJSON_CreateStringArray
  - >> cJSON_AddStringToObject

  cJSON_AddStringToObject (Thumb, 48 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = cJSON_AddStringToObject ⇒ add_item_to_object ⇒ cJSON_strdup
  [Calls]
  - >> cJSON_CreateString
  - >> cJSON_Delete
  - >> add_item_to_object
  [Called By]
  - >> exchange_results

  cJSON_CreateRaw (Thumb, 46 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_Delete
  - >> cJSON_New_Item
  - >> cJSON_strdup
  [Called By]
  - >> cJSON_AddRawToObject

  cJSON_AddRawToObject (Thumb, 48 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateRaw
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateObject (Thumb, 20 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = cJSON_CreateObject ⇒ cJSON_New_Item
  [Calls]
  - >> cJSON_New_Item
  [Called By]
  - >> exchange_results
  - >> cJSON_AddObjectToObject

  cJSON_AddObjectToObject (Thumb, 44 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateObject
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_CreateArray (Thumb, 20 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = cJSON_CreateArray ⇒ cJSON_New_Item
  [Calls]
  - >> cJSON_New_Item
  [Called By]
  - >> exchange_results
  - >> cJSON_CreateStringArray
  - >> cJSON_CreateDoubleArray
  - >> cJSON_CreateFloatArray
  - >> cJSON_CreateIntArray
  - >> cJSON_AddArrayToObject

  cJSON_AddArrayToObject (Thumb, 44 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateArray
  - >> cJSON_Delete
  - >> add_item_to_object

  cJSON_DetachItemViaPointer (Thumb, 74 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_DetachItemFromObjectCaseSensitive
  - >> cJSON_DetachItemFromObject
  - >> cJSON_DetachItemFromArray

  cJSON_DetachItemFromArray (Thumb, 34 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemViaPointer
  - >> get_array_item
  [Called By]
  - >> cJSON_DeleteItemFromArray

  cJSON_DeleteItemFromArray (Thumb, 22 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemFromArray
  - >> cJSON_Delete

  cJSON_DetachItemFromObject (Thumb, 26 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemViaPointer
  - >> cJSON_GetObjectItem
  [Called By]
  - >> cJSON_DeleteItemFromObject

  cJSON_DetachItemFromObjectCaseSensitive (Thumb, 26 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemViaPointer
  - >> cJSON_GetObjectItemCaseSensitive
  [Called By]
  - >> cJSON_DeleteItemFromObjectCaseSensitive

  cJSON_DeleteItemFromObject (Thumb, 22 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemFromObject
  - >> cJSON_Delete

  cJSON_DeleteItemFromObjectCaseSensitive (Thumb, 22 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_DetachItemFromObjectCaseSensitive
  - >> cJSON_Delete

  cJSON_InsertItemInArray (Thumb, 86 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> add_item_to_array
  - >> get_array_item

  cJSON_ReplaceItemViaPointer (Thumb, 100 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_Delete
  [Called By]
  - >> cJSON_ReplaceItemInArray
  - >> replace_item_in_object

  cJSON_ReplaceItemInArray (Thumb, 42 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_ReplaceItemViaPointer
  - >> get_array_item

  cJSON_ReplaceItemInObject (Thumb, 22 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> replace_item_in_object

  cJSON_ReplaceItemInObjectCaseSensitive (Thumb, 22 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> replace_item_in_object

  cJSON_CreateStringReference (Thumb, 32 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cast_away_const
  - >> cJSON_New_Item

  cJSON_CreateObjectReference (Thumb, 32 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cast_away_const
  - >> cJSON_New_Item

  cJSON_CreateArrayReference (Thumb, 32 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cast_away_const
  - >> cJSON_New_Item

  cJSON_CreateIntArray (Thumb, 110 bytes, Stack size 40 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_i2d
  - >> cJSON_CreateArray
  - >> cJSON_CreateNumber
  - >> cJSON_Delete
  - >> suffix_object

  cJSON_CreateFloatArray (Thumb, 110 bytes, Stack size 40 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_f2d
  - >> cJSON_CreateArray
  - >> cJSON_CreateNumber
  - >> cJSON_Delete
  - >> suffix_object

  cJSON_CreateDoubleArray (Thumb, 106 bytes, Stack size 32 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateArray
  - >> cJSON_CreateNumber
  - >> cJSON_Delete
  - >> suffix_object

  cJSON_CreateStringArray (Thumb, 100 bytes, Stack size 32 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_CreateArray
  - >> cJSON_CreateString
  - >> cJSON_Delete
  - >> suffix_object

  cJSON_Duplicate_rec (Thumb, 208 bytes, Stack size 32 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_Duplicate_rec
  - >> cJSON_Delete
  - >> cJSON_New_Item
  - >> cJSON_strdup
  [Called By]
  - >> cJSON_Duplicate
  - >> cJSON_Duplicate_rec

  cJSON_Duplicate (Thumb, 18 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_Duplicate_rec

  cJSON_Minify (Thumb, 154 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> minify_string
  - >> skip_multiline_comment
  - >> skip_oneline_comment

  cJSON_IsInvalid (Thumb, 20 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsFalse (Thumb, 20 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsTrue (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsBool (Thumb, 24 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> handle_param_exchange

  cJSON_IsNull (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsArray (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsObject (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_IsRaw (Thumb, 22 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)

  cJSON_Compare (Thumb, 384 bytes, Stack size 32 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> strcmp
  - >> cJSON_Compare
  - >> get_object_item
  - >> compare_double
  [Called By]
  - >> cJSON_Compare

  cJSON_malloc (Thumb, 14 bytes, Stack size 8 bytes, cjson.o(.text), UNUSED)

  stats_init (Thumb, 22 bytes, Stack size 0 bytes, iperf.o(.text))
  [Called By]

  - >> main

  stats_start (Thumb, 34 bytes, Stack size 8 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = stats_start ⇒ __2printf
  [Calls]
  - >> get_time_ms
  - >> __2printf
  [Called By]
  - >> start_iperf_test

  stats_update (Thumb, 184 bytes, Stack size 88 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = stats_update ⇒ __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_ui2d
  - >> __aeabi_ddiv
  - >> get_time_ms
  - >> __2printf
  [Called By]
  - >> start_iperf_test
  - >> stats_stop

  stats_stop (Thumb, 136 bytes, Stack size 56 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = stats_stop ⇒ stats_update ⇒ __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_ui2d
  - >> __aeabi_ddiv
  - >> stats_update
  - >> get_time_ms
  - >> __2printf
  [Called By]
  - >> start_iperf_test

  stats_add_bytes (Thumb, 34 bytes, Stack size 0 bytes, iperf.o(.text))
  [Called By]

  - >> start_iperf_test

  handle_param_exchange (Thumb, 318 bytes, Stack size 568 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 1000
  - Call Chain = handle_param_exchange ⇒ cJSON_Print ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> __aeabi_memclr4
  - >> send
  - >> recv
  - >> cJSON_IsBool
  - >> cJSON_GetObjectItem
  - >> cJSON_Print
  - >> cJSON_Parse
  - >> cJSON_Delete
  - >> cJSON_GetErrorPtr
  - >> __2printf
  [Called By]
  - >> main

  handle_create_streams (Thumb, 272 bytes, Stack size 48 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = handle_create_streams ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> socket
  - >> listen
  - >> getSn_RX_RSR
  - >> WIZCHIP_READ
  - >> sendto
  - >> send
  - >> recvfrom
  - >> recv
  - >> __2printf
  [Called By]
  - >> main

  exchange_results (Thumb, 1286 bytes, Stack size 1088 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 1520
  - Call Chain = exchange_results ⇒ cJSON_PrintUnformatted ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> strlen
  - >> send
  - >> recv
  - >> __aeabi_ui2d
  - >> __aeabi_ddiv
  - >> cJSON_CreateArray
  - >> cJSON_CreateObject
  - >> cJSON_AddStringToObject
  - >> cJSON_AddNumberToObject
  - >> cJSON_AddItemToObject
  - >> cJSON_AddItemToArray
  - >> cJSON_PrintUnformatted
  - >> cJSON_Delete
  - >> __2printf
  [Called By]
  - >> start_iperf_test

  start_iperf_test (Thumb, 292 bytes, Stack size 56 bytes, iperf.o(.text))
  [Stack]

  - Max Depth = 1576
  - Call Chain = start_iperf_test ⇒ exchange_results ⇒ cJSON_PrintUnformatted ⇒ print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> getSn_RX_RSR
  - >> sendto
  - >> send
  - >> recvfrom
  - >> recv
  - >> getsockopt
  - >> exchange_results
  - >> stats_add_bytes
  - >> stats_stop
  - >> stats_update
  - >> stats_start
  - >> __2printf
  [Called By]
  - >> main

  close (Thumb, 142 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> DHCP_stop
  - >> socket
  - >> listen
  - >> disconnect
  - >> main
  - >> send
  - >> recvfrom
  - >> recv

  socket (Thumb, 384 bytes, Stack size 24 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = socket ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> close
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> DHCP_run
  - >> handle_create_streams
  - >> main

  listen (Thumb, 158 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = listen ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> close
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> handle_create_streams
  - >> main

  connect (Thumb, 342 bytes, Stack size 16 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ

  disconnect (Thumb, 202 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = disconnect ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> close
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> main

  send (Thumb, 374 bytes, Stack size 24 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = send ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> close
  - >> wiz_send_data
  - >> getSn_TX_FSR
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test
  - >> handle_param_exchange
  - >> handle_create_streams
  - >> exchange_results

  recv (Thumb, 282 bytes, Stack size 32 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = recv ⇒ wiz_recv_data ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> close
  - >> wiz_recv_data
  - >> getSn_RX_RSR
  - >> getSn_TX_FSR
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test
  - >> handle_param_exchange
  - >> handle_create_streams
  - >> exchange_results

  sendto (Thumb, 530 bytes, Stack size 40 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wiz_send_data
  - >> getSn_TX_FSR
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test
  - >> handle_create_streams
  - >> check_DHCP_leasedIP
  - >> send_DHCP_DECLINE
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  recvfrom (Thumb, 768 bytes, Stack size 40 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = recvfrom ⇒ wiz_recv_data ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> close
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> getSn_RX_RSR
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test
  - >> handle_create_streams
  - >> parseDHCPMSG

  ctlsocket (Thumb, 308 bytes, Stack size 24 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ

  setsockopt (Thumb, 398 bytes, Stack size 16 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ

  getsockopt (Thumb, 408 bytes, Stack size 24 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = getsockopt ⇒ getSn_RX_RSR ⇒ WIZCHIP_READ
  [Calls]
  - >> getSn_RX_RSR
  - >> getSn_TX_FSR
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> start_iperf_test

  wizchip_cris_enter (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cris_exit (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cs_select (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cs_deselect (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_bus_readdata (Thumb, 6 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.data)

  wizchip_bus_writedata (Thumb, 4 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.data)

  wizchip_spi_readbyte (Thumb, 4 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_writebyte (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_readburst (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_writeburst (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  reg_wizchip_cris_cbfunc (Thumb, 30 bytes, Stack size 0 bytes, wizchip_conf.o(.text), UNUSED)

  reg_wizchip_cs_cbfunc (Thumb, 30 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  reg_wizchip_spi_cbfunc (Thumb, 44 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  reg_wizchip_spiburst_cbfunc (Thumb, 42 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  wizphy_getphylink (Thumb, 24 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = wizphy_getphylink ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_getphypmode (Thumb, 30 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = wizphy_getphypmode ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_reset (Thumb, 52 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip
  - >> wizphy_setphyconf
  - >> wizphy_setphypmode

  wizphy_setphypmode (Thumb, 100 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizphy_setphypmode ⇒ wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  - >> wizphy_reset
  [Called By]
  - >> ctlwizchip

  wizphy_getphyconf (Thumb, 120 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizphy_getphyconf ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_setphyconf (Thumb, 88 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizphy_setphyconf ⇒ wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> wizphy_reset
  [Called By]
  - >> ctlwizchip

  wizchip_getinterruptmask (Thumb, 40 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_getinterruptmask ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizchip_setinterruptmask (Thumb, 30 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_setinterruptmask ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  wizchip_getinterrupt (Thumb, 42 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_getinterrupt ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizchip_clrinterrupt (Thumb, 60 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_clrinterrupt ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  wizchip_sw_reset (Thumb, 114 bytes, Stack size 24 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = wizchip_sw_reset ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip
  - >> wizchip_init

  wizchip_init (Thumb, 144 bytes, Stack size 24 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_WRITE
  - >> wizchip_sw_reset
  [Called By]
  - >> ctlwizchip
  - >> main

  ctlwizchip (Thumb, 288 bytes, Stack size 32 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = ctlwizchip ⇒ wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> wizchip_init
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  - >> wizchip_sw_reset
  - >> wizchip_clrinterrupt
  - >> wizchip_getinterrupt
  - >> wizchip_setinterruptmask
  - >> wizchip_getinterruptmask
  - >> wizphy_setphyconf
  - >> wizphy_getphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> wizphy_getphypmode
  - >> wizphy_getphylink
  [Called By]
  - >> wiz_phy_link_check

  wizchip_gettimeout (Thumb, 40 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_settimeout (Thumb, 38 bytes, Stack size 8 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlnetwork

  wizchip_getnetmode (Thumb, 10 bytes, Stack size 8 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_setnetmode (Thumb, 38 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_getnetinfo (Thumb, 82 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_getnetinfo ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  [Called By]
  - >> print_network_information
  - >> main
  - >> ctlnetwork

  wizchip_setnetinfo (Thumb, 80 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_setnetinfo ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  [Called By]
  - >> wiz_dhcp_process
  - >> network_init
  - >> ctlnetwork

  ctlnetwork (Thumb, 80 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> wizchip_setnetinfo
  - >> wizchip_getnetinfo
  - >> wizchip_setnetmode
  - >> wizchip_getnetmode
  - >> wizchip_settimeout
  - >> wizchip_gettimeout

  wizphy_getphystat (Thumb, 28 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ

  default_ip_assign (Thumb, 38 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = default_ip_assign ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  [Called By]
  - >> default_ip_update
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  default_ip_update (Thumb, 34 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = default_ip_update ⇒ default_ip_assign ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  - >> default_ip_assign
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  default_ip_conflict (Thumb, 30 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = default_ip_conflict ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  reg_dhcp_cbfunc (Thumb, 46 bytes, Stack size 8 bytes, dhcp.o(.text), UNUSED)

  makeDHCPMSG (Thumb, 386 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = makeDHCPMSG ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  [Called By]
  - >> send_DHCP_DECLINE
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  NibbleToHex (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  send_DHCP_DISCOVER (Thumb, 688 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = send_DHCP_DISCOVER ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> NibbleToHex
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> DHCP_run
  - >> check_DHCP_timeout

  send_DHCP_REQUEST (Thumb, 1000 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = send_DHCP_REQUEST ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> NibbleToHex
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> DHCP_run
  - >> check_DHCP_timeout

  send_DHCP_DECLINE (Thumb, 492 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> check_DHCP_leasedIP

  parseDHCPMSG (Thumb, 636 bytes, Stack size 40 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = parseDHCPMSG ⇒ recvfrom ⇒ wiz_recv_data ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> getSn_RX_RSR
  - >> recvfrom
  [Called By]
  - >> DHCP_run

  reset_DHCP_timeout (Thumb, 20 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> DHCP_run
  - >> DHCP_init
  - >> check_DHCP_timeout

  check_DHCP_timeout (Thumb, 154 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = check_DHCP_timeout ⇒ send_DHCP_REQUEST ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> reset_DHCP_timeout
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER
  [Called By]
  - >> DHCP_run

  check_DHCP_leasedIP (Thumb, 88 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  - >> send_DHCP_DECLINE
  - >> sendto
  [Called By]
  - >> DHCP_run

  DHCP_run (Thumb, 424 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> socket
  - >> WIZCHIP_READ
  - >> check_DHCP_leasedIP
  - >> check_DHCP_timeout
  - >> reset_DHCP_timeout
  - >> parseDHCPMSG
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER
  [Called By]
  - >> wiz_dhcp_process

  DHCP_stop (Thumb, 18 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = DHCP_stop ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> close
  [Called By]
  - >> wiz_dhcp_process

  DHCP_init (Thumb, 294 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DHCP_init ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_WRITE_BUF
  - >> reset_DHCP_timeout
  [Called By]
  - >> wiz_dhcp_process

  DHCP_time_handler (Thumb, 12 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  getIPfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getGWfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getSNfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getDNSfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getDHCPLeasetime (Thumb, 6 bytes, Stack size 0 bytes, dhcp.o(.text), UNUSED)

  MH_RCC_PLLConfig (Thumb, 236 bytes, Stack size 32 bytes, mh.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MH_RCC_PLLConfig
  [Called By]
  - >> WIZ_RCC_PLLConfig

  MH_LSE_DriveConfig (Thumb, 74 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)

  MH_PLL_SelLockConfig (Thumb, 128 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)

  MH_PLL_CpConfig (Thumb, 96 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)

  MH_FLASH_FastProgramPage (Thumb, 374 bytes, Stack size 56 bytes, mh.o(.text), UNUSED)

  tolower (Thumb, 12 bytes, Stack size 0 bytes, tolower.o(.text))
  [Called By]

  - >> case_insensitive_strcmp

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> wiz_read_buff
  - >> wiz_write_buff
  - >> print
  - >> print_value
  - >> print_string_ptr
  - >> ensure
  - >> cJSON_strdup
  - >> internal_alloc

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)
  [Called By]

  - >> create_reference

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> wiz_read_buff
  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> handle_param_exchange
  - >> cJSON_PrintPreallocated
  - >> cJSON_PrintBuffered
  - >> cJSON_ParseWithLengthOpts
  - >> print
  - >> print_number
  - >> cJSON_New_Item

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> exchange_results
  - >> cJSON_ParseWithOpts
  - >> cJSON_SetValuestring
  - >> print_value
  - >> update_offset
  - >> cJSON_strdup

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> cJSON_Compare
  - >> get_object_item

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> cJSON_SetValuestring
  - >> print_value
  - >> print_string_ptr

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> parse_value
  - >> skip_utf8_bom

  __0sscanf (Thumb, 48 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> print_number

  _scanf_real (Thumb, 0 bytes, Stack size 104 bytes, scanf_fp.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = _scanf_real
  [Called By]
  - >> __vfscanf
  - >> _local_sscanf

  _scanf_really_real (Thumb, 556 bytes, Stack size 104 bytes, scanf_fp.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_d2f
  - >> _is_digit
  - >> _fp_value

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> compare_double

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> compare_double
  - >> _fp_value
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> exchange_results
  - >> stats_stop
  - >> stats_update
  - >> _fp_value
  - >> _fp_digits

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> cJSON_CreateIntArray
  - >> print_number

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> exchange_results
  - >> stats_stop
  - >> stats_update

  __aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2iz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> cJSON_CreateNumber
  - >> cJSON_SetNumberHelper
  - >> parse_number

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text), UNUSED)
  [Called By]

  - >> cJSON_CreateFloatArray

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> print_number

  __aeabi_cdcmple (Thumb, 48 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> cJSON_CreateNumber
  - >> cJSON_SetNumberHelper
  - >> compare_double
  - >> parse_number

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> cJSON_CreateNumber
  - >> cJSON_SetNumberHelper
  - >> compare_double
  - >> parse_number
  - >> _fp_digits

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2iz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __vfscanf_char (Thumb, 20 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 2]

  - __0sscanf.o(.text)
  - strtod.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 2]

  - __0sscanf.o(.text)
  - strtod.o(.text)

  __strtod_int (Thumb, 90 bytes, Stack size 40 bytes, strtod.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> _local_sscanf
  [Called By]
  - >> strtod

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> _double_epilogue
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_ul2d
  - >> __aeabi_dadd

  __aeabi_ul2d (Thumb, 24 bytes, Stack size 16 bytes, dfltul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_value

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text), UNUSED)
  [Calls]

  - >> _float_round
  [Called By]
  - >> _scanf_really_real

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  isspace (Thumb, 10 bytes, Stack size 0 bytes, isspace_c.o(.text))
  [Calls]

  - >> __ctype_lookup
  [Address Reference Count : 2]
  - scanf_char.o(.text)
  - strtod.o(.text)

  __vfscanf (Thumb, 808 bytes, Stack size 88 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = __vfscanf ⇒ _scanf_real
  [Calls]
  - >> _scanf_real
  [Called By]
  - >> __vfscanf_char

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_d2f

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text), UNUSED)

  __ctype_lookup (Thumb, 34 bytes, Stack size 0 bytes, ctype_c.o(.text))
  [Called By]

  - >> isspace

  WIZ_RCC_PLLConfig (Thumb, 28 bytes, Stack size 24 bytes, w55mh32.o(.text.WIZ_RCC_PLLConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = WIZ_RCC_PLLConfig ⇒ MH_RCC_PLLConfig
  [Calls]
  - >> MH_RCC_PLLConfig
  [Called By]
  - >> rcc_clk_config

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> print_network_information
  - >> wiz_print_phy_info
  - >> wiz_dhcp_process
  - >> wiz_phy_link_check
  - >> start_iperf_test
  - >> handle_param_exchange
  - >> handle_create_streams
  - >> main
  - >> exchange_results
  - >> stats_stop
  - >> stats_update
  - >> stats_start

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> cJSON_Version
  - >> print_string_ptr
  - >> print_number

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  free (Thumb, 88 bytes, Stack size 12 bytes, mallocr.o(i.__free$realloc))
  [Stack]

  - Max Depth = 12
  - Call Chain = free
  [Called By]
  - >> realloc
  [Address Reference Count : 2]
  - cjson.o(.data)
  - cjson.o(.text)

  malloc (Thumb, 64 bytes, Stack size 32 bytes, mallocr.o(i.__malloc$realloc))
  [Stack]

  - Max Depth = 56
  - Call Chain = malloc ⇒ internal_alloc
  [Calls]
  - >> internal_alloc
  [Called By]
  - >> realloc
  [Address Reference Count : 2]
  - cjson.o(.data)
  - cjson.o(.text)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, scanf_fp.o(i._is_digit), UNUSED)
  [Called By]

  - >> _scanf_really_real

  realloc (Thumb, 102 bytes, Stack size 32 bytes, mallocr.o(i.realloc))
  [Stack]

  - Max Depth = 88
  - Call Chain = realloc ⇒ malloc ⇒ internal_alloc
  [Calls]
  - >> malloc
  - >> free
  - >> internal_alloc
  [Address Reference Count : 2]
  - cjson.o(.data)
  - cjson.o(.text)

  strtod (Thumb, 28 bytes, Stack size 16 bytes, strtod.o(i.strtod))
  [Stack]

  - Max Depth = 216
  - Call Chain = strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> __strtod_int
  [Called By]
  - >> parse_number

  ### Local Symbols

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 108 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  wiztoe_delay (Thumb, 34 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiztoe_delay
  [Called By]
  - >> wiz_toe_init
  - >> wiztoe_hw_reset

  spi_dma_init (Thumb, 122 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> DMA_ITConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> RCC_AHBPeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> wiztoe_bus_init
  - >> spi_dma_transfer

  spi_dma_transfer (Thumb, 352 bytes, Stack size 112 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = spi_dma_transfer ⇒ spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> DMA_Init
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> spi_dma_init
  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  [Called By]
  - >> wiz_read_buff
  - >> wiz_write_buff

  wiz_write_byte (Thumb, 48 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiz_write_byte
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_SendData
  [Called By]
  - >> wiz_write_buff
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiz_read_byte (Thumb, 62 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiz_read_byte
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_SendData
  [Called By]
  - >> wiz_read_buff
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiz_write_buff (Thumb, 92 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = wiz_write_buff ⇒ spi_dma_transfer ⇒ spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> wiz_write_byte
  - >> spi_dma_transfer
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiz_read_buff (Thumb, 102 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = wiz_read_buff ⇒ spi_dma_transfer ⇒ spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> wiz_read_byte
  - >> spi_dma_transfer
  - >> __aeabi_memset
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiz_select (Thumb, 48 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiz_select
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiz_deselect (Thumb, 48 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = wiz_deselect
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - w55mh32_wztoe.o(.text)

  wiztoe_bus_init (Thumb, 216 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = wiztoe_bus_init ⇒ spi_dma_init ⇒ NVIC_Init
  [Calls]
  - >> spi_dma_init
  - >> SPI_I2S_ClearFlag
  - >> SPI_Cmd
  - >> SPI_Init
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> wiz_toe_init

  wiztoe_hw_reset (Thumb, 88 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wiztoe_hw_reset ⇒ GPIO_Init
  [Calls]
  - >> wiztoe_delay
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> wiz_toe_init

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  wiz_dhcp_process (Thumb, 146 bytes, Stack size 48 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = wiz_dhcp_process ⇒ DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_setnetinfo
  - >> getSNfromDHCP
  - >> getIPfromDHCP
  - >> getGWfromDHCP
  - >> getDNSfromDHCP
  - >> DHCP_stop
  - >> DHCP_run
  - >> DHCP_init
  - >> WIZCHIP_READ_BUF
  - >> __2printf
  [Called By]
  - >> network_init

  case_insensitive_strcmp (Thumb, 72 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = case_insensitive_strcmp
  [Calls]
  - >> tolower
  [Called By]
  - >> get_object_item

  cJSON_strdup (Thumb, 56 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = cJSON_strdup
  [Calls]
  - >> strlen
  - >> __aeabi_memcpy
  [Called By]
  - >> cJSON_Duplicate_rec
  - >> cJSON_CreateRaw
  - >> cJSON_CreateString
  - >> cJSON_SetValuestring
  - >> replace_item_in_object
  - >> add_item_to_object

  cJSON_New_Item (Thumb, 26 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = cJSON_New_Item
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> cJSON_Duplicate_rec
  - >> cJSON_CreateArrayReference
  - >> cJSON_CreateObjectReference
  - >> cJSON_CreateStringReference
  - >> cJSON_CreateArray
  - >> cJSON_CreateObject
  - >> cJSON_CreateRaw
  - >> cJSON_CreateString
  - >> cJSON_CreateNumber
  - >> cJSON_CreateBool
  - >> cJSON_CreateFalse
  - >> cJSON_CreateTrue
  - >> cJSON_CreateNull
  - >> cJSON_ParseWithLengthOpts
  - >> create_reference
  - >> parse_array
  - >> parse_object

  get_decimal_point (Thumb, 4 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> print_number
  - >> parse_number

  parse_number (Thumb, 298 bytes, Stack size 96 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 312
  - Call Chain = parse_number ⇒ strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> strtod
  - >> __aeabi_d2iz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> get_decimal_point
  [Called By]
  - >> parse_value

  ensure (Thumb, 240 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = ensure
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> print_value
  - >> print_array
  - >> print_object
  - >> print_string_ptr
  - >> print_number

  update_offset (Thumb, 36 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = update_offset
  [Calls]
  - >> strlen
  [Called By]
  - >> print
  - >> print_array
  - >> print_object

  compare_double (Thumb, 112 bytes, Stack size 48 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = compare_double ⇒ __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  [Called By]
  - >> cJSON_Compare
  - >> print_number

  print_number (Thumb, 304 bytes, Stack size 80 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 344
  - Call Chain = print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_i2d
  - >> __aeabi_cdcmpeq
  - >> compare_double
  - >> ensure
  - >> get_decimal_point
  - >> __0sscanf
  - >> __2sprintf
  [Called By]
  - >> print_value

  parse_hex4 (Thumb, 90 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> utf16_literal_to_utf8

  utf16_literal_to_utf8 (Thumb, 300 bytes, Stack size 56 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = utf16_literal_to_utf8
  [Calls]
  - >> parse_hex4
  [Called By]
  - >> parse_string

  parse_string (Thumb, 438 bytes, Stack size 40 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = parse_string ⇒ utf16_literal_to_utf8
  [Calls]
  - >> utf16_literal_to_utf8
  [Called By]
  - >> parse_value
  - >> parse_object

  print_string_ptr (Thumb, 360 bytes, Stack size 32 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = print_string_ptr ⇒ ensure
  [Calls]
  - >> strcpy
  - >> __aeabi_memcpy
  - >> ensure
  - >> __2sprintf
  [Called By]
  - >> print_object
  - >> print_string

  print_string (Thumb, 16 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = print_string ⇒ print_string_ptr ⇒ ensure
  [Calls]
  - >> print_string_ptr
  [Called By]
  - >> print_value

  buffer_skip_whitespace (Thumb, 72 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> cJSON_ParseWithLengthOpts
  - >> parse_array
  - >> parse_object

  skip_utf8_bom (Thumb, 56 bytes, Stack size 8 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = skip_utf8_bom ⇒ strncmp
  [Calls]
  - >> strncmp
  [Called By]
  - >> cJSON_ParseWithLengthOpts

  parse_object (Thumb, 332 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 120 + In Cycle
  - Call Chain = parse_object ⇒ parse_value (Cycle)
  [Calls]
  - >> cJSON_Delete
  - >> parse_value
  - >> buffer_skip_whitespace
  - >> parse_string
  - >> cJSON_New_Item
  [Called By]
  - >> parse_value

  parse_array (Thumb, 266 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 40 + In Cycle
  - Call Chain = parse_array ⇒ parse_value (Cycle)
  [Calls]
  - >> cJSON_Delete
  - >> parse_value
  - >> buffer_skip_whitespace
  - >> cJSON_New_Item
  [Called By]
  - >> parse_value

  parse_value (Thumb, 292 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 328
  - Call Chain = parse_value ⇒ parse_number ⇒ strtod ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> strncmp
  - >> parse_array
  - >> parse_object
  - >> parse_string
  - >> parse_number
  [Called By]
  - >> cJSON_ParseWithLengthOpts
  - >> parse_array
  - >> parse_object

  print_object (Thumb, 372 bytes, Stack size 32 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 88 + In Cycle
  - Call Chain = print_object ⇒ print_value (Cycle)
  [Calls]
  - >> print_value
  - >> print_string_ptr
  - >> update_offset
  - >> ensure
  [Called By]
  - >> print_value

  print_array (Thumb, 204 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = print_array ⇒ print_value (Cycle)
  [Calls]
  - >> print_value
  - >> update_offset
  - >> ensure
  [Called By]
  - >> print_value

  print_value (Thumb, 242 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> strcpy
  - >> strlen
  - >> __aeabi_memcpy
  - >> print_array
  - >> print_object
  - >> print_string
  - >> print_number
  - >> ensure
  [Called By]
  - >> cJSON_PrintPreallocated
  - >> cJSON_PrintBuffered
  - >> print
  - >> print_array
  - >> print_object

  print (Thumb, 188 bytes, Stack size 56 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 424
  - Call Chain = print ⇒ print_value ⇒ print_number ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_real
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> print_value
  - >> update_offset
  [Called By]
  - >> cJSON_PrintUnformatted
  - >> cJSON_Print

  get_array_item (Thumb, 30 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_ReplaceItemInArray
  - >> cJSON_InsertItemInArray
  - >> cJSON_DetachItemFromArray
  - >> cJSON_GetArrayItem

  get_object_item (Thumb, 82 bytes, Stack size 24 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = get_object_item ⇒ case_insensitive_strcmp
  [Calls]
  - >> strcmp
  - >> case_insensitive_strcmp
  [Called By]
  - >> cJSON_Compare
  - >> cJSON_GetObjectItemCaseSensitive
  - >> cJSON_GetObjectItem
  - >> replace_item_in_object

  suffix_object (Thumb, 6 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> cJSON_CreateStringArray
  - >> cJSON_CreateDoubleArray
  - >> cJSON_CreateFloatArray
  - >> cJSON_CreateIntArray
  - >> add_item_to_array

  create_reference (Thumb, 60 bytes, Stack size 16 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4
  - >> cJSON_New_Item
  [Called By]
  - >> cJSON_AddItemReferenceToObject
  - >> cJSON_AddItemReferenceToArray

  add_item_to_array (Thumb, 54 bytes, Stack size 16 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = add_item_to_array
  [Calls]
  - >> suffix_object
  [Called By]
  - >> cJSON_InsertItemInArray
  - >> cJSON_AddItemReferenceToArray
  - >> cJSON_AddItemToArray
  - >> add_item_to_object

  cast_away_const (Thumb, 2 bytes, Stack size 0 bytes, cjson.o(.text))
  [Called By]

  - >> cJSON_CreateArrayReference
  - >> cJSON_CreateObjectReference
  - >> cJSON_CreateStringReference
  - >> add_item_to_object

  add_item_to_object (Thumb, 122 bytes, Stack size 32 bytes, cjson.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = add_item_to_object ⇒ cJSON_strdup
  [Calls]
  - >> cast_away_const
  - >> add_item_to_array
  - >> cJSON_strdup
  [Called By]
  - >> cJSON_AddArrayToObject
  - >> cJSON_AddObjectToObject
  - >> cJSON_AddRawToObject
  - >> cJSON_AddStringToObject
  - >> cJSON_AddNumberToObject
  - >> cJSON_AddBoolToObject
  - >> cJSON_AddFalseToObject
  - >> cJSON_AddTrueToObject
  - >> cJSON_AddNullToObject
  - >> cJSON_AddItemReferenceToObject
  - >> cJSON_AddItemToObjectCS
  - >> cJSON_AddItemToObject

  replace_item_in_object (Thumb, 108 bytes, Stack size 24 bytes, cjson.o(.text), UNUSED)
  [Calls]

  - >> cJSON_ReplaceItemViaPointer
  - >> cJSON_free
  - >> get_object_item
  - >> cJSON_strdup
  [Called By]
  - >> cJSON_ReplaceItemInObjectCaseSensitive
  - >> cJSON_ReplaceItemInObject

  skip_oneline_comment (Thumb, 42 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_Minify

  skip_multiline_comment (Thumb, 50 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_Minify

  minify_string (Thumb, 120 bytes, Stack size 0 bytes, cjson.o(.text), UNUSED)
  [Called By]

  - >> cJSON_Minify

  _fp_digits (Thumb, 366 bytes, Stack size 64 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_ddiv
  - >> __aeabi_dmul
  - >> __aeabi_cdrcmple
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  internal_alloc (Thumb, 76 bytes, Stack size 24 bytes, mallocr.o(i.internal_alloc))
  [Stack]

  - Max Depth = 24
  - Call Chain = internal_alloc
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> realloc
  - >> malloc

  _fp_value (Thumb, 296 bytes, Stack size 64 bytes, scanf_fp.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_ddiv
  - >> __aeabi_dmul
  - >> __aeabi_ul2d
  [Called By]
  - >> _scanf_really_real

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  _local_sscanf (Thumb, 54 bytes, Stack size 56 bytes, strtod.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = _local_sscanf ⇒ _scanf_real
  [Calls]
  - >> _scanf_real
  [Called By]
  - >> __strtod_int

  ### Undefined Global Symbols