# Static Call Graph for image ..\Output\Project.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Fri Dec 26 16:55:35 2025

### Maximum Stack Usage = 11712 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ httpServer_run ⇒ http_process_handler ⇒ http_post_cgi_handler ⇒ predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- disk_write ⇒ disk_write
- disk_read ⇒ disk_read

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - ADC3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - BusFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_RX1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - CAN1_SCE_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - DebugMon_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - EP1_IN_Callback from usb_endp.o(.text) referenced 2 times from usb_istr.o(.data)
  - EP3_OUT_Callback from usb_endp.o(.text) referenced 2 times from usb_istr.o(.data)
  - EXTI0_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI15_10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - EXTI9_5_IRQHandler from user_gpio.o(.text) referenced from startup_w55mh32.o(RESET)
  - FLASH_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - FSMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - HardFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C1_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_ER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - I2C2_EV_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - MemManage_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - NMI_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - NOP_Process from usb_core.o(.text) referenced 38 times from usb_istr.o(.data)
  - PVD_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - PendSV_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - RCC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RNG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTCAlarm_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - RTC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - Reset_Handler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SDIO_IRQHandler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SENSOR_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SPI3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - SVC_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SYMC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - Standard_GetConfiguration from usb_core.o(.text) referenced from usb_core.o(.text)
  - Standard_GetInterface from usb_core.o(.text) referenced from usb_core.o(.text)
  - Standard_GetStatus from usb_core.o(.text) referenced 3 times from usb_core.o(.text)
  - SysTick_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - SystemInit from system_w55mh32.o(.text) referenced from startup_w55mh32.o(.text)
  - TAMPER_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM3_IRQHandler from bsp_tim.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM6_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM7_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_CC_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART4_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - UART5_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART1_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART2_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USART3_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USBWakeUp_IRQHandler from hw_config.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from hw_config.o(.text) referenced from startup_w55mh32.o(RESET)
  - UsageFault_Handler from w55mh32_it.o(.text) referenced from startup_w55mh32.o(RESET)
  - Virtual_Com_Port_Data_Setup from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetConfigDescriptor from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetDeviceDescriptor from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetLineCoding from usb_prop.o(.text) referenced from usb_prop.o(.text)
  - Virtual_Com_Port_GetStringDescriptor from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Get_Interface_Setting from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_NoData_Setup from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Reset from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetConfiguration from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetDeviceAddress from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetLineCoding from usb_prop.o(.text) referenced from usb_prop.o(.text)
  - Virtual_Com_Port_Status_In from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Status_Out from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_init from usb_prop.o(.text) referenced 2 times from usb_prop.o(.data)
  - WWDG_IRQHandler from startup_w55mh32.o(.text) referenced from startup_w55mh32.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_w55mh32.o(.text)
  - _sbackspace from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0vsprintf)
  - default_ip_assign from dhcp.o(.text) referenced 2 times from dhcp.o(.data)
  - default_ip_assign from dhcp.o(.text) referenced from dhcp.o(.text)
  - default_ip_conflict from dhcp.o(.text) referenced 2 times from dhcp.o(.data)
  - default_ip_conflict from dhcp.o(.text) referenced from dhcp.o(.text)
  - default_ip_update from dhcp.o(.text) referenced 2 times from dhcp.o(.data)
  - default_ip_update from dhcp.o(.text) referenced from dhcp.o(.text)
  - default_mcu_reset from httpserver.o(.text) referenced 2 times from httpserver.o(.data)
  - default_wdt_reset from httpserver.o(.text) referenced 2 times from httpserver.o(.data)
  - fputc from bsp_uart.o(.text) referenced from printfa.o(i.__0printf)
  - isspace from isspace_c.o(.text) referenced from scanf_char.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - wizchip_bus_readdata from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_bus_writedata from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_cris_enter from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_cris_enter from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cris_exit from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_cris_exit from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cs_deselect from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_cs_deselect from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_cs_select from wizchip_conf.o(.text) referenced 2 times from wizchip_conf.o(.data)
  - wizchip_cs_select from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_readburst from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_readbyte from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_writeburst from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)
  - wizchip_spi_writebyte from wizchip_conf.o(.text) referenced from wizchip_conf.o(.text)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_w55mh32.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  BOOT_RAM (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SENSOR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SYMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_w55mh32.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> usb_init
  - >> NVIC_Configuration

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> user_gpio_init
  - >> tim3_init
  - >> USB_Interrupts_Config
  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> rcc_clk_config
  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> Set_USBClock

  RCC_ADCCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> rcc_clk_config

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 230 bytes, Stack size 20 bytes, w55mh32_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> tim3_init
  - >> delay_init
  - >> I2S_Init
  - >> USART_Init
  - >> wiztoe_bus_init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> SD_DeInit
  - >> GPIO_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> user_gpio_init
  - >> i2c_CfgGpio
  - >> console_usart_init
  - >> MYI2C_Init
  - >> USB_Port_Set
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init
  - >> GPIO_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text))
  [Called By]

  - >> tim3_init
  - >> Set_USBClock
  - >> wiztoe_bus_init

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, w55mh32_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> user_gpio_init
  - >> i2c_CfgGpio
  - >> console_usart_init
  - >> MYI2C_GPIO_MODE
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init
  - >> SD_DeInit
  - >> GPIO_Configuration

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text))
  [Called By]

  - >> MYI2C_GPIO_DATA
  - >> EXTI9_5_IRQHandler
  - >> TIM3_IRQHandler

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text))
  [Called By]

  - >> user_gpio_init
  - >> MYI2C_GPIO_DATA
  - >> led_off
  - >> beep_on
  - >> wiztoe_hw_reset
  - >> wiztoe_bus_init
  - >> wiz_deselect

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text))
  [Called By]

  - >> MYI2C_GPIO_DATA
  - >> led_on
  - >> beep_off
  - >> wiztoe_hw_reset
  - >> wiz_select

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfigUser (Thumb, 50 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, w55mh32_gpio.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = GPIO_EXTILineConfig
  [Called By]
  - >> user_gpio_init

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForcePuPdCmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForcePullUpConfig (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  GPIO_ForceDropDownConfig (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_gpio.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 230 bytes, Stack size 56 bytes, w55mh32_usart.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> console_usart_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> console_usart_init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 104 bytes, Stack size 16 bytes, w55mh32_usart.o(.text), UNUSED)

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, w55mh32_usart.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, w55mh32_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, w55mh32_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> wiztoe_bus_init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, w55mh32_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text))
  [Called By]

  - >> wiztoe_bus_init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)
  [Called By]

  - >> wiz_write_byte
  - >> wiz_read_byte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)
  [Called By]

  - >> wiz_write_byte
  - >> wiz_read_byte

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)
  [Called By]

  - >> wiz_write_byte
  - >> wiz_read_byte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, w55mh32_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_spi.o(.text), UNUSED)

  TIM_DeInit (Thumb, 346 bytes, Stack size 8 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 104 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_OC1Init (Thumb, 114 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 150 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 114 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 78 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 150 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> tim3_init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 32 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 82 bytes, Stack size 16 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, w55mh32_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM3_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  EXTI_DeInit (Thumb, 28 bytes, Stack size 0 bytes, w55mh32_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 142 bytes, Stack size 0 bytes, w55mh32_exti.o(.text))
  [Called By]

  - >> user_gpio_init
  - >> USB_Interrupts_Config

  EXTI_StructInit (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 34 bytes, Stack size 0 bytes, w55mh32_exti.o(.text))
  [Called By]

  - >> EXTI9_5_IRQHandler

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_exti.o(.text))
  [Called By]

  - >> USB_Interrupts_Config
  - >> EXTI9_5_IRQHandler
  - >> USBWakeUp_IRQHandler

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_Init (Thumb, 60 bytes, Stack size 8 bytes, w55mh32_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> SD_DMA_TxConfig
  - >> SD_DMA_RxConfig

  DMA_StructInit (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 24 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> SD_DMA_TxConfig
  - >> SD_DMA_RxConfig

  DMA_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 40 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> SD_DMAEndOfTransferStatus

  DMA_ClearFlag (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_dma.o(.text))
  [Called By]

  - >> SD_DMA_TxConfig
  - >> SD_DMA_RxConfig

  DMA_GetITStatus (Thumb, 40 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_dma.o(.text), UNUSED)

  SDIO_DeInit (Thumb, 28 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_DeInit
  - >> SD_Init

  SDIO_Init (Thumb, 42 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_PowerON
  - >> SD_EnableWideBusOperation
  - >> SD_Init

  SDIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_ClockCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_PowerON
  - >> SD_DeInit

  SDIO_SetPowerState (Thumb, 22 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_PowerOFF
  - >> SD_PowerON
  - >> SD_DeInit

  SDIO_GetPowerState (Thumb, 10 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_InitializeCards

  SDIO_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_DMACmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_SendCommand (Thumb, 38 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_Erase
  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_SendSDStatus
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_SelectDeselect
  - >> IsCardProgramming
  - >> SDEnWideBus
  - >> FindSCR
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_CmdStructInit (Thumb, 14 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_GetCommandResponse (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> IsCardProgramming
  - >> CmdResp6Error

  SDIO_GetResponse (Thumb, 22 bytes, Stack size 8 bytes, w55mh32_sdio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SDIO_GetResponse
  [Called By]
  - >> SD_Erase
  - >> SD_SendSDStatus
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> IsCardProgramming
  - >> CmdResp6Error
  - >> SDEnWideBus

  SDIO_DataConfig (Thumb, 42 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_SendSDStatus
  - >> FindSCR
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  SDIO_DataStructInit (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_GetDataCounter (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_ReadData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_SendSDStatus
  - >> FindSCR

  SDIO_WriteData (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_GetFIFOCount (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_StartSDIOReadWait (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_StopSDIOReadWait (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_SetSDIOReadWaitMode (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_SetSDIOOperation (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_SendSDIOSuspendCmd (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_CommandCompletionCmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_CEATAITCmd (Thumb, 12 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_SendCEATACmd (Thumb, 8 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_GetFlagStatus (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_SendSDStatus
  - >> CmdError
  - >> FindSCR

  SDIO_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_SendSDStatus
  - >> IsCardProgramming
  - >> CmdError
  - >> CmdResp7Error
  - >> CmdResp3Error
  - >> CmdResp6Error
  - >> CmdResp2Error
  - >> FindSCR
  - >> SD_WaitWriteOperation

  SDIO_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text), UNUSED)

  SDIO_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, w55mh32_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc

  main (Thumb, 192 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 11712
  - Call Chain = main ⇒ httpServer_run ⇒ http_process_handler ⇒ http_post_cgi_handler ⇒ predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> wizchip_getnetinfo
  - >> wiz_toe_init
  - >> wiz_phy_link_check
  - >> user_gpio_init
  - >> usb_run
  - >> usb_init
  - >> tim3_init
  - >> reg_httpServer_webContent
  - >> rcc_clk_config
  - >> network_init
  - >> i2c_CfgGpio
  - >> httpServer_run
  - >> httpServer_init
  - >> delay_ms
  - >> delay_init
  - >> console_usart_init
  - >> check_eeprom_network_info
  - >> MYI2C_Init
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_w55mh32.o(.text)

  SystemCoreClockUpdate (Thumb, 160 bytes, Stack size 8 bytes, system_w55mh32.o(.text), UNUSED)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, w55mh32_it.o(.text))
  [Address Reference Count : 1]

  - startup_w55mh32.o(RESET)

  SDIO_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, w55mh32_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SDIO_IRQHandler ⇒ SD_ProcessIRQSrc
  [Calls]
  - >> SD_ProcessIRQSrc
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  wiz_print_phy_info (Thumb, 54 bytes, Stack size 8 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wiz_print_phy_info ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  - >> __2printf
  [Called By]
  - >> wiz_phy_link_check

  wiz_phy_link_check (Thumb, 56 bytes, Stack size 8 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = wiz_phy_link_check ⇒ ctlwizchip ⇒ wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> delay_ms
  - >> ctlwizchip
  - >> wiz_print_phy_info
  - >> __2printf
  [Called By]
  - >> main

  print_network_information (Thumb, 190 bytes, Stack size 40 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = print_network_information ⇒ wizchip_getnetinfo ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> wizchip_getnetinfo
  - >> __2printf
  [Called By]
  - >> network_init

  network_init (Thumb, 46 bytes, Stack size 16 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = network_init ⇒ wiz_dhcp_process ⇒ DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_setnetinfo
  - >> print_network_information
  - >> wiz_dhcp_process
  [Called By]
  - >> main

  tim3_init (Thumb, 112 bytes, Stack size 40 bytes, bsp_tim.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = tim3_init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_GetClocksFreq
  - >> NVIC_Init
  [Called By]
  - >> main

  TIM3_IRQHandler (Thumb, 138 bytes, Stack size 8 bytes, bsp_tim.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = TIM3_IRQHandler ⇒ MYI2C_Handle ⇒ MYI2C_READ_FUNC ⇒ MYI2C_Read_IIC_Byte ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> GPIO_ReadInputDataBit
  - >> httpServer_time_handler
  - >> MYI2C_Handle
  - >> DHCP_time_handler
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  console_usart_init (Thumb, 118 bytes, Stack size 32 bytes, bsp_uart.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = console_usart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Cmd
  - >> USART_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  fputc (Thumb, 32 bytes, Stack size 16 bytes, bsp_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  delay_init (Thumb, 76 bytes, Stack size 24 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = delay_init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> i2c_Delay

  delay_ms (Thumb, 126 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> wiz_phy_link_check
  - >> usb_init
  - >> main

  i2c_Stop (Thumb, 28 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_Stop ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> i2c_CfgGpio
  - >> ee_WriteBytes
  - >> ee_ReadBytes
  - >> ee_CheckDevice

  i2c_CfgGpio (Thumb, 44 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = i2c_CfgGpio ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> i2c_Stop
  [Called By]
  - >> main

  i2c_Start (Thumb, 40 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_Start ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_WriteBytes
  - >> ee_ReadBytes
  - >> ee_CheckDevice

  i2c_SendByte (Thumb, 80 bytes, Stack size 16 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = i2c_SendByte ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_WriteBytes
  - >> ee_ReadBytes
  - >> ee_CheckDevice

  i2c_ReadByte (Thumb, 62 bytes, Stack size 16 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = i2c_ReadByte ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_ReadBytes

  i2c_WaitAck (Thumb, 58 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_WaitAck ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_WriteBytes
  - >> ee_ReadBytes
  - >> ee_CheckDevice

  i2c_Ack (Thumb, 44 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_Ack ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_ReadBytes

  i2c_NAck (Thumb, 38 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_NAck ⇒ i2c_Delay
  [Calls]
  - >> i2c_Delay
  [Called By]
  - >> ee_ReadBytes
  - >> ee_CheckDevice

  ee_CheckDevice (Thumb, 32 bytes, Stack size 16 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ee_CheckDevice ⇒ i2c_SendByte ⇒ i2c_Delay
  [Calls]
  - >> i2c_NAck
  - >> i2c_WaitAck
  - >> i2c_SendByte
  - >> i2c_Start
  - >> i2c_Stop
  [Called By]
  - >> check_eeprom_network_info
  - >> ee_WaitStandby

  ee_WaitStandby (Thumb, 34 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = ee_WaitStandby ⇒ ee_CheckDevice ⇒ i2c_SendByte ⇒ i2c_Delay
  [Calls]
  - >> ee_CheckDevice
  [Called By]
  - >> ee_WriteBytes

  ee_ReadBytes (Thumb, 112 bytes, Stack size 24 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = ee_ReadBytes ⇒ i2c_ReadByte ⇒ i2c_Delay
  [Calls]
  - >> i2c_NAck
  - >> i2c_Ack
  - >> i2c_WaitAck
  - >> i2c_ReadByte
  - >> i2c_SendByte
  - >> i2c_Start
  - >> i2c_Stop
  [Called By]
  - >> check_eeprom_network_info

  ee_WriteBytes (Thumb, 138 bytes, Stack size 32 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = ee_WriteBytes ⇒ ee_WaitStandby ⇒ ee_CheckDevice ⇒ i2c_SendByte ⇒ i2c_Delay
  [Calls]
  - >> ee_WaitStandby
  - >> i2c_WaitAck
  - >> i2c_SendByte
  - >> i2c_Start
  - >> i2c_Stop
  [Called By]
  - >> set_netinfo
  - >> ee_Erase

  ee_Erase (Thumb, 56 bytes, Stack size 264 bytes, eeprom.o(.text), UNUSED)
  [Calls]

  - >> ee_WriteBytes
  - >> __2printf

  check_eeprom_network_info (Thumb, 86 bytes, Stack size 32 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = check_eeprom_network_info ⇒ ee_ReadBytes ⇒ i2c_ReadByte ⇒ i2c_Delay
  [Calls]
  - >> ee_ReadBytes
  - >> ee_CheckDevice
  - >> __2printf
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  [Called By]
  - >> main

  make_json_update_page (Thumb, 226 bytes, Stack size 304 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 328
  - Call Chain = make_json_update_page ⇒ __2sprintf
  [Calls]
  - >> __aeabi_f2d
  - >> __2sprintf
  - >> __2printf
  - >> strcat
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  [Called By]
  - >> predefined_get_cgi_processor

  make_json_netinfo (Thumb, 118 bytes, Stack size 96 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = make_json_netinfo ⇒ wizchip_getnetinfo ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> wizchip_getnetinfo
  - >> __2sprintf
  [Called By]
  - >> predefined_get_cgi_processor

  predefined_get_cgi_processor (Thumb, 228 bytes, Stack size 280 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 6176
  - Call Chain = predefined_get_cgi_processor ⇒ get_sd_filename ⇒ f_opendir ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> get_sd_filename
  - >> make_json_netinfo
  - >> make_json_update_page
  - >> __2sprintf
  - >> __2printf
  - >> strcmp
  - >> strcat
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  [Called By]
  - >> http_get_cgi_handler

  set_netinfo (Thumb, 184 bytes, Stack size 136 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 392
  - Call Chain = set_netinfo ⇒ parse_ip ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> wizchip_getnetinfo
  - >> get_http_param_value
  - >> parse_ip
  - >> ee_WriteBytes
  - >> __2sprintf
  - >> strcpy
  [Called By]
  - >> predefined_set_cgi_processor

  predefined_set_cgi_processor (Thumb, 762 bytes, Stack size 288 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 10096
  - Call Chain = predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> usb_printf
  - >> put_sd
  - >> led_on
  - >> led_off
  - >> get_http_param_value
  - >> beep_on
  - >> beep_off
  - >> ATOI
  - >> set_netinfo
  - >> __2sprintf
  - >> strcpy
  - >> strcmp
  [Called By]
  - >> http_post_cgi_handler

  user_gpio_init (Thumb, 144 bytes, Stack size 24 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = user_gpio_init ⇒ GPIO_Init
  [Calls]
  - >> EXTI_Init
  - >> GPIO_EXTILineConfig
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  led_on (Thumb, 14 bytes, Stack size 8 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = led_on
  [Calls]
  - >> GPIO_ResetBits
  [Called By]
  - >> predefined_set_cgi_processor

  led_off (Thumb, 14 bytes, Stack size 8 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = led_off
  [Calls]
  - >> GPIO_SetBits
  [Called By]
  - >> predefined_set_cgi_processor

  beep_on (Thumb, 14 bytes, Stack size 8 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = beep_on
  [Calls]
  - >> GPIO_SetBits
  [Called By]
  - >> predefined_set_cgi_processor

  beep_off (Thumb, 14 bytes, Stack size 8 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = beep_off
  [Calls]
  - >> GPIO_ResetBits
  [Called By]
  - >> predefined_set_cgi_processor

  EXTI9_5_IRQHandler (Thumb, 42 bytes, Stack size 8 bytes, user_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI9_5_IRQHandler
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> GPIO_ReadInputDataBit
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  MYI2C_Delay_us (Thumb, 24 bytes, Stack size 0 bytes, aht20.o(.text))
  [Called By]

  - >> MYI2C_Init
  - >> MYI2C_READ_FUNC
  - >> MYI2C_Read_IIC_Byte
  - >> MYI2C_Write_IIC_Byte
  - >> MYI2C_IIC_Wait_Ack
  - >> MYI2C_IIC_Ack
  - >> MYI2C_IIC_Stop
  - >> MYI2C_IIC_Start

  MYI2C_GPIO_MODE (Thumb, 104 bytes, Stack size 16 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> MYI2C_Init
  - >> MYI2C_Read_IIC_Byte
  - >> MYI2C_IIC_Wait_Ack

  MYI2C_GPIO_DATA (Thumb, 78 bytes, Stack size 16 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = MYI2C_GPIO_DATA
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> MYI2C_Init
  - >> MYI2C_READ_FUNC
  - >> MYI2C_Read_IIC_Byte
  - >> MYI2C_Write_IIC_Byte
  - >> MYI2C_IIC_Wait_Ack
  - >> MYI2C_IIC_Ack
  - >> MYI2C_IIC_Stop
  - >> MYI2C_IIC_Start

  MYI2C_IIC_Start (Thumb, 52 bytes, Stack size 8 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = MYI2C_IIC_Start ⇒ MYI2C_GPIO_DATA
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_WRITE_FUNC
  - >> MYI2C_READ_FUNC

  MYI2C_IIC_Stop (Thumb, 52 bytes, Stack size 8 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = MYI2C_IIC_Stop ⇒ MYI2C_GPIO_DATA
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_WRITE_FUNC
  - >> MYI2C_READ_FUNC

  MYI2C_IIC_Ack (Thumb, 58 bytes, Stack size 8 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = MYI2C_IIC_Ack ⇒ MYI2C_GPIO_DATA
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_READ_FUNC

  MYI2C_IIC_Wait_Ack (Thumb, 82 bytes, Stack size 8 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = MYI2C_IIC_Wait_Ack ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_GPIO_MODE
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_WRITE_FUNC
  - >> MYI2C_READ_FUNC

  MYI2C_Write_IIC_Byte (Thumb, 78 bytes, Stack size 16 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MYI2C_Write_IIC_Byte ⇒ MYI2C_GPIO_DATA
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_WRITE_FUNC
  - >> MYI2C_READ_FUNC

  MYI2C_Read_IIC_Byte (Thumb, 100 bytes, Stack size 16 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = MYI2C_Read_IIC_Byte ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_GPIO_MODE
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_READ_FUNC

  MYI2C_Init (Thumb, 76 bytes, Stack size 16 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = MYI2C_Init ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_GPIO_MODE
  - >> MYI2C_Delay_us
  [Called By]
  - >> main

  MYI2C_READ_FUNC (Thumb, 164 bytes, Stack size 32 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = MYI2C_READ_FUNC ⇒ MYI2C_Read_IIC_Byte ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> MYI2C_Read_IIC_Byte
  - >> MYI2C_Write_IIC_Byte
  - >> MYI2C_IIC_Wait_Ack
  - >> MYI2C_IIC_Ack
  - >> MYI2C_IIC_Stop
  - >> MYI2C_IIC_Start
  - >> MYI2C_GPIO_DATA
  - >> MYI2C_Delay_us
  [Called By]
  - >> MYI2C_Handle

  MYI2C_WRITE_FUNC (Thumb, 98 bytes, Stack size 32 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = MYI2C_WRITE_FUNC ⇒ MYI2C_IIC_Wait_Ack ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> MYI2C_Write_IIC_Byte
  - >> MYI2C_IIC_Wait_Ack
  - >> MYI2C_IIC_Stop
  - >> MYI2C_IIC_Start
  [Called By]
  - >> MYI2C_Handle

  CheckCrc8 (Thumb, 58 bytes, Stack size 12 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CheckCrc8
  [Called By]
  - >> MYI2C_Handle

  MYI2C_Handle (Thumb, 262 bytes, Stack size 24 bytes, aht20.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = MYI2C_Handle ⇒ MYI2C_READ_FUNC ⇒ MYI2C_Read_IIC_Byte ⇒ MYI2C_GPIO_MODE ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> CheckCrc8
  - >> MYI2C_WRITE_FUNC
  - >> MYI2C_READ_FUNC
  [Called By]
  - >> TIM3_IRQHandler

  rcc_clk_config (Thumb, 124 bytes, Stack size 8 bytes, user_rcc.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = rcc_clk_config ⇒ WIZ_RCC_PLLConfig ⇒ MH_RCC_PLLConfig
  [Calls]
  - >> RCC_LSICmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HCLKConfig
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLCmd
  - >> RCC_HSICmd
  - >> RCC_GetFlagStatus
  - >> RCC_HSEConfig
  - >> RCC_DeInit
  - >> WIZ_RCC_PLLConfig
  [Called By]
  - >> main

  usb_init (Thumb, 58 bytes, Stack size 8 bytes, user_usb.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = usb_init ⇒ USB_Interrupts_Config ⇒ NVIC_Init
  [Calls]
  - >> delay_ms
  - >> NVIC_PriorityGroupConfig
  - >> USB_Port_Set
  - >> USB_Interrupts_Config
  - >> USB_Init
  - >> Set_USBClock
  [Called By]
  - >> main

  usb_run (Thumb, 146 bytes, Stack size 8 bytes, user_usb.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = usb_run ⇒ usb_printf ⇒ vsprintf
  [Calls]
  - >> usb_printf
  - >> __2printf
  - >> strncpy
  [Called By]
  - >> main

  get_sd_filename (Thumb, 194 bytes, Stack size 4496 bytes, user_sdio.o(.text))
  [Stack]

  - Max Depth = 5896
  - Call Chain = get_sd_filename ⇒ f_opendir ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> f_readdir
  - >> f_opendir
  - >> f_mount
  - >> __2printf
  - >> strcpy
  - >> strcmp
  [Called By]
  - >> predefined_get_cgi_processor

  put_sd (Thumb, 114 bytes, Stack size 8344 bytes, user_sdio.o(.text))
  [Stack]

  - Max Depth = 9808
  - Call Chain = put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> f_write
  - >> f_open
  - >> f_mount
  - >> f_close
  - >> __2printf
  [Called By]
  - >> predefined_set_cgi_processor

  close (Thumb, 142 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> recvfrom
  - >> recv
  - >> send
  - >> disconnect
  - >> listen
  - >> socket
  - >> DHCP_stop

  socket (Thumb, 384 bytes, Stack size 24 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = socket ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run
  - >> DHCP_run

  listen (Thumb, 158 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = listen ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run

  connect (Thumb, 342 bytes, Stack size 16 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ

  disconnect (Thumb, 202 bytes, Stack size 8 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = disconnect ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run

  send (Thumb, 374 bytes, Stack size 24 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = send ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wiz_send_data
  - >> getSn_TX_FSR
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ
  [Called By]
  - >> send_http_response_cgi
  - >> send_http_response_header
  - >> send_http_response_body

  recv (Thumb, 282 bytes, Stack size 32 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = recv ⇒ wiz_recv_data ⇒ WIZCHIP_WRITE
  [Calls]
  - >> wiz_recv_data
  - >> getSn_TX_FSR
  - >> getSn_RX_RSR
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run

  sendto (Thumb, 530 bytes, Stack size 40 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wiz_send_data
  - >> getSn_TX_FSR
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> check_DHCP_leasedIP
  - >> send_DHCP_DECLINE
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  recvfrom (Thumb, 768 bytes, Stack size 40 bytes, socket.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = recvfrom ⇒ wiz_recv_data ⇒ WIZCHIP_WRITE
  [Calls]
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> getSn_RX_RSR
  - >> WIZCHIP_WRITE
  - >> close
  - >> WIZCHIP_READ
  [Called By]
  - >> parseDHCPMSG

  ctlsocket (Thumb, 308 bytes, Stack size 24 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ

  setsockopt (Thumb, 398 bytes, Stack size 16 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ

  getsockopt (Thumb, 408 bytes, Stack size 24 bytes, socket.o(.text), UNUSED)
  [Calls]

  - >> getSn_TX_FSR
  - >> getSn_RX_RSR
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ

  wizchip_cris_enter (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cris_exit (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cs_select (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_cs_deselect (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 2]

  - wizchip_conf.o(.text)
  - wizchip_conf.o(.data)

  wizchip_bus_readdata (Thumb, 6 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.data)

  wizchip_bus_writedata (Thumb, 4 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.data)

  wizchip_spi_readbyte (Thumb, 4 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_writebyte (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_readburst (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  wizchip_spi_writeburst (Thumb, 2 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Address Reference Count : 1]

  - wizchip_conf.o(.text)

  reg_wizchip_cris_cbfunc (Thumb, 30 bytes, Stack size 0 bytes, wizchip_conf.o(.text), UNUSED)

  reg_wizchip_cs_cbfunc (Thumb, 30 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  reg_wizchip_spi_cbfunc (Thumb, 44 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  reg_wizchip_spiburst_cbfunc (Thumb, 42 bytes, Stack size 0 bytes, wizchip_conf.o(.text))
  [Called By]

  - >> wiz_toe_init

  wizphy_getphylink (Thumb, 24 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizphy_getphylink ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_getphypmode (Thumb, 30 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizphy_getphypmode ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_reset (Thumb, 52 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> wizphy_setphyconf
  - >> wizphy_setphypmode
  - >> ctlwizchip

  wizphy_setphypmode (Thumb, 100 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = wizphy_setphypmode ⇒ wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> wizphy_reset
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_getphyconf (Thumb, 120 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizphy_getphyconf ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizphy_setphyconf (Thumb, 88 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = wizphy_setphyconf ⇒ wizphy_reset ⇒ WIZCHIP_WRITE
  [Calls]
  - >> wizphy_reset
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  wizchip_getinterruptmask (Thumb, 40 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizchip_getinterruptmask ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizchip_setinterruptmask (Thumb, 30 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizchip_setinterruptmask ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  wizchip_getinterrupt (Thumb, 42 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizchip_getinterrupt ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlwizchip

  wizchip_clrinterrupt (Thumb, 60 bytes, Stack size 16 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizchip_clrinterrupt ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  wizchip_sw_reset (Thumb, 114 bytes, Stack size 24 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = wizchip_sw_reset ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> wizchip_init
  - >> ctlwizchip

  wizchip_init (Thumb, 144 bytes, Stack size 24 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_sw_reset
  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlwizchip

  ctlwizchip (Thumb, 288 bytes, Stack size 32 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = ctlwizchip ⇒ wizchip_init ⇒ wizchip_sw_reset ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_init
  - >> wizchip_sw_reset
  - >> wizchip_clrinterrupt
  - >> wizchip_getinterrupt
  - >> wizchip_setinterruptmask
  - >> wizchip_getinterruptmask
  - >> wizphy_setphyconf
  - >> wizphy_getphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> wizphy_getphypmode
  - >> wizphy_getphylink
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> wiz_phy_link_check

  wizchip_gettimeout (Thumb, 40 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_settimeout (Thumb, 38 bytes, Stack size 8 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  [Called By]
  - >> ctlnetwork

  wizchip_getnetmode (Thumb, 10 bytes, Stack size 8 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_setnetmode (Thumb, 38 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> ctlnetwork

  wizchip_getnetinfo (Thumb, 82 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = wizchip_getnetinfo ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  [Called By]
  - >> main
  - >> ctlnetwork
  - >> set_netinfo
  - >> make_json_netinfo
  - >> print_network_information

  wizchip_setnetinfo (Thumb, 80 bytes, Stack size 8 bytes, wizchip_conf.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = wizchip_setnetinfo ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  [Called By]
  - >> network_init
  - >> ctlnetwork
  - >> wiz_dhcp_process

  ctlnetwork (Thumb, 80 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> wizchip_getnetinfo
  - >> wizchip_setnetmode
  - >> wizchip_getnetmode
  - >> wizchip_settimeout
  - >> wizchip_gettimeout
  - >> wizchip_setnetinfo

  wizphy_getphystat (Thumb, 28 bytes, Stack size 16 bytes, wizchip_conf.o(.text), UNUSED)
  [Calls]

  - >> WIZCHIP_READ

  default_ip_assign (Thumb, 38 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = default_ip_assign ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  [Called By]
  - >> default_ip_update
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  default_ip_update (Thumb, 34 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = default_ip_update ⇒ default_ip_assign ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> default_ip_assign
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  default_ip_conflict (Thumb, 30 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = default_ip_conflict ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Address Reference Count : 2]
  - dhcp.o(.data)
  - dhcp.o(.text)

  reg_dhcp_cbfunc (Thumb, 46 bytes, Stack size 8 bytes, dhcp.o(.text), UNUSED)

  makeDHCPMSG (Thumb, 386 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = makeDHCPMSG ⇒ WIZCHIP_READ_BUF
  [Calls]
  - >> WIZCHIP_READ_BUF
  [Called By]
  - >> send_DHCP_DECLINE
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  NibbleToHex (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER

  send_DHCP_DISCOVER (Thumb, 688 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = send_DHCP_DISCOVER ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> NibbleToHex
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> check_DHCP_timeout
  - >> DHCP_run

  send_DHCP_REQUEST (Thumb, 1000 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = send_DHCP_REQUEST ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> NibbleToHex
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> check_DHCP_timeout
  - >> DHCP_run

  send_DHCP_DECLINE (Thumb, 492 bytes, Stack size 24 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> makeDHCPMSG
  - >> sendto
  [Called By]
  - >> check_DHCP_leasedIP

  parseDHCPMSG (Thumb, 636 bytes, Stack size 40 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = parseDHCPMSG ⇒ recvfrom ⇒ wiz_recv_data ⇒ WIZCHIP_WRITE
  [Calls]
  - >> getSn_RX_RSR
  - >> recvfrom
  [Called By]
  - >> DHCP_run

  reset_DHCP_timeout (Thumb, 20 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> check_DHCP_timeout
  - >> DHCP_run
  - >> DHCP_init

  check_DHCP_timeout (Thumb, 154 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = check_DHCP_timeout ⇒ send_DHCP_REQUEST ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> reset_DHCP_timeout
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER
  [Called By]
  - >> DHCP_run

  check_DHCP_leasedIP (Thumb, 88 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> send_DHCP_DECLINE
  - >> WIZCHIP_WRITE
  - >> sendto
  - >> WIZCHIP_READ
  [Called By]
  - >> DHCP_run

  DHCP_run (Thumb, 424 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> check_DHCP_leasedIP
  - >> check_DHCP_timeout
  - >> reset_DHCP_timeout
  - >> parseDHCPMSG
  - >> send_DHCP_REQUEST
  - >> send_DHCP_DISCOVER
  - >> socket
  - >> WIZCHIP_READ
  [Called By]
  - >> wiz_dhcp_process

  DHCP_stop (Thumb, 18 bytes, Stack size 8 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DHCP_stop ⇒ close ⇒ WIZCHIP_WRITE
  [Calls]
  - >> close
  [Called By]
  - >> wiz_dhcp_process

  DHCP_init (Thumb, 294 bytes, Stack size 16 bytes, dhcp.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = DHCP_init ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> reset_DHCP_timeout
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_READ_BUF
  [Called By]
  - >> wiz_dhcp_process

  DHCP_time_handler (Thumb, 12 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  getIPfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getGWfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getSNfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getDNSfromDHCP (Thumb, 26 bytes, Stack size 0 bytes, dhcp.o(.text))
  [Called By]

  - >> wiz_dhcp_process

  getDHCPLeasetime (Thumb, 6 bytes, Stack size 0 bytes, dhcp.o(.text), UNUSED)

  unescape_http_url (Thumb, 62 bytes, Stack size 24 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = unescape_http_url
  [Calls]
  - >> C2D
  [Called By]
  - >> get_http_param_value

  make_http_response_head (Thumb, 182 bytes, Stack size 32 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = make_http_response_head ⇒ __2sprintf
  [Calls]
  - >> __2sprintf
  - >> strcpy
  - >> strcat
  [Called By]
  - >> send_http_response_header

  find_http_uri_type (Thumb, 1234 bytes, Stack size 16 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = find_http_uri_type ⇒ strstr
  [Calls]
  - >> strstr
  [Called By]
  - >> http_process_handler

  parse_http_request (Thumb, 162 bytes, Stack size 16 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = parse_http_request ⇒ strtok
  [Calls]
  - >> strtok
  - >> strcpy
  - >> strcmp
  [Called By]
  - >> httpServer_run

  ATOI (Thumb, 36 bytes, Stack size 16 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = ATOI
  [Calls]
  - >> C2D
  [Called By]
  - >> inet_addr_
  - >> get_http_param_value
  - >> predefined_set_cgi_processor

  mid (Thumb, 68 bytes, Stack size 32 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = mid ⇒ strstr
  [Calls]
  - >> strlen
  - >> strncpy
  - >> strstr
  [Called By]
  - >> http_process_handler
  - >> get_http_param_value

  get_http_param_value (Thumb, 182 bytes, Stack size 48 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = get_http_param_value ⇒ mid ⇒ strstr
  [Calls]
  - >> mid
  - >> unescape_http_url
  - >> replacetochar
  - >> ATOI
  - >> strlen
  - >> strncpy
  - >> strstr
  [Called By]
  - >> predefined_set_cgi_processor
  - >> set_netinfo

  get_http_uri_name (Thumb, 54 bytes, Stack size 16 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = get_http_uri_name ⇒ strtok
  [Calls]
  - >> strtok
  - >> strcpy
  - >> strcmp
  [Called By]
  - >> http_process_handler

  inet_addr_ (Thumb, 92 bytes, Stack size 56 bytes, httpparser.o(.text), UNUSED)
  [Calls]

  - >> ATOI
  - >> strtok
  - >> strcpy

  default_mcu_reset (Thumb, 2 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Address Reference Count : 1]

  - httpserver.o(.data)

  default_wdt_reset (Thumb, 2 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Address Reference Count : 1]

  - httpserver.o(.data)

  httpServer_Sockinit (Thumb, 24 bytes, Stack size 8 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = httpServer_Sockinit
  [Called By]
  - >> httpServer_init

  httpServer_init (Thumb, 28 bytes, Stack size 20 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = httpServer_init ⇒ httpServer_Sockinit
  [Calls]
  - >> httpServer_Sockinit
  [Called By]
  - >> main

  reg_httpServer_cbfunc (Thumb, 14 bytes, Stack size 0 bytes, httpserver.o(.text), UNUSED)

  read_userReg_webContent (Thumb, 76 bytes, Stack size 32 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = read_userReg_webContent ⇒ strncpy
  [Calls]
  - >> strlen
  - >> strncpy
  [Called By]
  - >> send_http_response_body

  get_httpServer_timecount (Thumb, 6 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Called By]

  - >> httpServer_run

  find_userReg_webContent (Thumb, 78 bytes, Stack size 24 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = find_userReg_webContent ⇒ strcmp
  [Calls]
  - >> strcmp
  [Called By]
  - >> http_process_handler

  httpServer_run (Thumb, 1320 bytes, Stack size 40 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 11680
  - Call Chain = httpServer_run ⇒ http_process_handler ⇒ http_post_cgi_handler ⇒ predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> get_httpServer_timecount
  - >> http_process_handler
  - >> send_http_response_body
  - >> http_disconnect
  - >> getHTTPSocketNum
  - >> parse_http_request
  - >> getSn_TX_FSR
  - >> getSn_RX_RSR
  - >> WIZCHIP_WRITE
  - >> recv
  - >> disconnect
  - >> listen
  - >> socket
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ
  - >> __2printf
  [Called By]
  - >> main

  httpServer_time_handler (Thumb, 12 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  reg_httpServer_webContent (Thumb, 124 bytes, Stack size 24 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = reg_httpServer_webContent ⇒ malloc
  [Calls]
  - >> malloc
  - >> strcpy
  - >> strlen
  [Called By]
  - >> main

  display_reg_webContent_list (Thumb, 136 bytes, Stack size 16 bytes, httpserver.o(.text), UNUSED)
  [Calls]

  - >> __2printf

  http_get_cgi_handler (Thumb, 50 bytes, Stack size 24 bytes, httputil.o(.text))
  [Stack]

  - Max Depth = 6200
  - Call Chain = http_get_cgi_handler ⇒ predefined_get_cgi_processor ⇒ get_sd_filename ⇒ f_opendir ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> predefined_get_cgi_processor
  - >> strcmp
  [Called By]
  - >> http_process_handler

  http_post_cgi_handler (Thumb, 78 bytes, Stack size 32 bytes, httputil.o(.text))
  [Stack]

  - Max Depth = 10128
  - Call Chain = http_post_cgi_handler ⇒ predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> predefined_set_cgi_processor
  - >> __2sprintf
  - >> strcmp
  [Called By]
  - >> http_process_handler

  USBWakeUp_IRQHandler (Thumb, 12 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBWakeUp_IRQHandler
  [Calls]
  - >> EXTI_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = USB_LP_CAN1_RX0_IRQHandler ⇒ USB_Istr ⇒ CTR_LP ⇒ Setup0_Process ⇒ Data_Setup0 ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> USB_Istr
  [Address Reference Count : 1]
  - startup_w55mh32.o(RESET)

  Set_USBClock (Thumb, 18 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Set_USBClock
  [Calls]
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_USBCLKConfig
  [Called By]
  - >> usb_init

  Enter_LowPowerMode (Thumb, 16 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Enter_LowPowerMode ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> Suspend

  Leave_LowPowerMode (Thumb, 30 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Leave_LowPowerMode ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> Resume_Init

  USB_Interrupts_Config (Thumb, 90 bytes, Stack size 16 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_Interrupts_Config ⇒ NVIC_Init
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_Init
  - >> NVIC_Init
  [Called By]
  - >> usb_init

  USB_Cable_Config (Thumb, 22 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_Cable_Config ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> PowerOff
  - >> PowerOn

  USB_Port_Set (Thumb, 74 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_Port_Set
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> usb_init

  IntToUnicode (Thumb, 62 bytes, Stack size 12 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = IntToUnicode
  [Called By]
  - >> Get_SerialNum

  Get_SerialNum (Thumb, 42 bytes, Stack size 16 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Get_SerialNum ⇒ IntToUnicode
  [Calls]
  - >> IntToUnicode
  [Called By]
  - >> Virtual_Com_Port_init

  USART_Config (Thumb, 62 bytes, Stack size 8 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = USART_Config ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> Virtual_Com_Port_Status_In

  USB_To_USART_Send_Data (Thumb, 120 bytes, Stack size 12 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_To_USART_Send_Data
  [Called By]
  - >> EP3_OUT_Callback

  USB_USART_SendData (Thumb, 42 bytes, Stack size 0 bytes, hw_config.o(.text))
  [Called By]

  - >> usb_printf

  usb_printf (Thumb, 56 bytes, Stack size 32 bytes, hw_config.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = usb_printf ⇒ vsprintf
  [Calls]
  - >> USB_USART_SendData
  - >> vsprintf
  - >> strlen
  [Called By]
  - >> usb_run
  - >> predefined_set_cgi_processor

  EP1_IN_Callback (Thumb, 188 bytes, Stack size 8 bytes, usb_endp.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = EP1_IN_Callback ⇒ UserToPMABufferCopy
  [Calls]
  - >> UserToPMABufferCopy
  - >> SetEPTxValid
  - >> SetEPTxCount
  [Called By]
  - >> SOF_Callback
  [Address Reference Count : 1]
  - usb_istr.o(.data)

  EP3_OUT_Callback (Thumb, 28 bytes, Stack size 8 bytes, usb_endp.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = EP3_OUT_Callback ⇒ USB_SIL_Read ⇒ PMAToUserBufferCopy
  [Calls]
  - >> USB_SIL_Read
  - >> SetEPRxValid
  - >> USB_To_USART_Send_Data
  [Address Reference Count : 1]
  - usb_istr.o(.data)

  SOF_Callback (Thumb, 38 bytes, Stack size 8 bytes, usb_endp.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = SOF_Callback ⇒ EP1_IN_Callback ⇒ UserToPMABufferCopy
  [Calls]
  - >> EP1_IN_Callback
  [Called By]
  - >> USB_Istr

  USB_Istr (Thumb, 426 bytes, Stack size 40 bytes, usb_istr.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = USB_Istr ⇒ CTR_LP ⇒ Setup0_Process ⇒ Data_Setup0 ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> Suspend
  - >> Resume
  - >> CTR_LP
  - >> SOF_Callback
  [Called By]
  - >> USB_LP_CAN1_RX0_IRQHandler

  Virtual_Com_Port_init (Thumb, 30 bytes, Stack size 8 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Virtual_Com_Port_init ⇒ PowerOn ⇒ USB_Cable_Config ⇒ __2printf
  [Calls]
  - >> USB_SIL_Init
  - >> PowerOn
  - >> Get_SerialNum
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_Reset (Thumb, 216 bytes, Stack size 8 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Virtual_Com_Port_Reset ⇒ SetEPTxStatus
  [Calls]
  - >> SetEPType
  - >> SetEPTxStatus
  - >> SetEPTxAddr
  - >> SetEPRxStatus
  - >> SetEPRxCount
  - >> SetEPRxAddr
  - >> SetDeviceAddress
  - >> SetBTABLE
  - >> Clear_Status_Out
  - >> SetEPRxValid
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_SetConfiguration (Thumb, 14 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_SetDeviceAddress (Thumb, 8 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_Status_In (Thumb, 22 bytes, Stack size 8 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Virtual_Com_Port_Status_In ⇒ USART_Config ⇒ __2printf
  [Calls]
  - >> USART_Config
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_Status_Out (Thumb, 2 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_SetLineCoding (Thumb, 20 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.text)

  Virtual_Com_Port_GetLineCoding (Thumb, 20 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.text)

  Virtual_Com_Port_Data_Setup (Thumb, 86 bytes, Stack size 16 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Virtual_Com_Port_Data_Setup
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_NoData_Setup (Thumb, 36 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_GetDeviceDescriptor (Thumb, 14 bytes, Stack size 8 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Virtual_Com_Port_GetDeviceDescriptor ⇒ Standard_GetDescriptorData
  [Calls]
  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_GetConfigDescriptor (Thumb, 14 bytes, Stack size 8 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Virtual_Com_Port_GetConfigDescriptor ⇒ Standard_GetDescriptorData
  [Calls]
  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_GetStringDescriptor (Thumb, 32 bytes, Stack size 16 bytes, usb_prop.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Virtual_Com_Port_GetStringDescriptor ⇒ Standard_GetDescriptorData
  [Calls]
  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_Get_Interface_Setting (Thumb, 22 bytes, Stack size 0 bytes, usb_prop.o(.text))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  PowerOn (Thumb, 54 bytes, Stack size 8 bytes, usb_pwr.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = PowerOn ⇒ USB_Cable_Config ⇒ __2printf
  [Calls]
  - >> USB_Cable_Config
  [Called By]
  - >> Virtual_Com_Port_init

  PowerOff (Thumb, 28 bytes, Stack size 8 bytes, usb_pwr.o(.text), UNUSED)
  [Calls]

  - >> USB_Cable_Config

  Suspend (Thumb, 142 bytes, Stack size 16 bytes, usb_pwr.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Suspend ⇒ Enter_LowPowerMode ⇒ __2printf
  [Calls]
  - >> Enter_LowPowerMode
  [Called By]
  - >> USB_Istr

  Resume_Init (Thumb, 30 bytes, Stack size 8 bytes, usb_pwr.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Resume_Init ⇒ Leave_LowPowerMode ⇒ __2printf
  [Calls]
  - >> Leave_LowPowerMode
  [Called By]
  - >> Resume

  Resume (Thumb, 194 bytes, Stack size 16 bytes, usb_pwr.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Resume ⇒ Resume_Init ⇒ Leave_LowPowerMode ⇒ __2printf
  [Calls]
  - >> Resume_Init
  [Called By]
  - >> USB_Istr

  Standard_GetConfiguration (Thumb, 34 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_GetConfiguration
  [Address Reference Count : 1]
  - usb_core.o(.text)

  Standard_SetConfiguration (Thumb, 60 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_SetConfiguration
  [Called By]
  - >> NoData_Setup0

  Standard_GetInterface (Thumb, 34 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_GetInterface
  [Address Reference Count : 1]
  - usb_core.o(.text)

  Standard_SetInterface (Thumb, 96 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_SetInterface
  [Called By]
  - >> NoData_Setup0

  Standard_GetStatus (Thumb, 238 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_GetStatus
  [Address Reference Count : 1]
  - usb_core.o(.text)

  Standard_ClearFeature (Thumb, 342 bytes, Stack size 32 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = Standard_ClearFeature ⇒ SetEPTxStatus
  [Calls]
  - >> ClearDTOG_TX
  - >> ClearDTOG_RX
  - >> SetEPTxStatus
  - >> SetEPRxCount
  [Called By]
  - >> NoData_Setup0

  Standard_SetEndPointFeature (Thumb, 220 bytes, Stack size 24 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Standard_SetEndPointFeature
  [Called By]
  - >> NoData_Setup0

  Standard_SetDeviceFeature (Thumb, 30 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_SetDeviceFeature
  [Called By]
  - >> NoData_Setup0

  Standard_GetDescriptorData (Thumb, 32 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Standard_GetDescriptorData
  [Called By]
  - >> Virtual_Com_Port_GetStringDescriptor
  - >> Virtual_Com_Port_GetConfigDescriptor
  - >> Virtual_Com_Port_GetDeviceDescriptor

  Post0_Process (Thumb, 54 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Post0_Process ⇒ SetEPRxCount
  [Calls]
  - >> SetEPRxCount
  [Called By]
  - >> Out0_Process
  - >> In0_Process
  - >> Setup0_Process

  Setup0_Process (Thumb, 170 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = Setup0_Process ⇒ Data_Setup0 ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> ByteSwap
  - >> Post0_Process
  - >> Data_Setup0
  - >> NoData_Setup0
  [Called By]
  - >> CTR_LP

  SetDeviceAddress (Thumb, 70 bytes, Stack size 12 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetDeviceAddress
  [Called By]
  - >> In0_Process
  - >> Virtual_Com_Port_Reset

  In0_Process (Thumb, 98 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = In0_Process ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> Post0_Process
  - >> DataStageIn
  - >> SetDeviceAddress
  [Called By]
  - >> CTR_LP

  Out0_Process (Thumb, 70 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Out0_Process ⇒ DataStageOut ⇒ PMAToUserBufferCopy
  [Calls]
  - >> Post0_Process
  - >> DataStageOut
  [Called By]
  - >> CTR_LP

  NOP_Process (Thumb, 2 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Address Reference Count : 2]

  - usb_prop.o(.data)
  - usb_istr.o(.data)

  USB_Init (Thumb, 36 bytes, Stack size 8 bytes, usb_init.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_Init
  [Called By]
  - >> usb_init

  CTR_LP (Thumb, 682 bytes, Stack size 16 bytes, usb_int.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = CTR_LP ⇒ Setup0_Process ⇒ Data_Setup0 ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> Out0_Process
  - >> In0_Process
  - >> Setup0_Process
  [Called By]
  - >> USB_Istr

  CTR_HP (Thumb, 178 bytes, Stack size 8 bytes, usb_int.o(.text), UNUSED)

  UserToPMABufferCopy (Thumb, 52 bytes, Stack size 20 bytes, usb_mem.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = UserToPMABufferCopy
  [Called By]
  - >> USB_SIL_Write
  - >> DataStageIn
  - >> EP1_IN_Callback

  PMAToUserBufferCopy (Thumb, 34 bytes, Stack size 20 bytes, usb_mem.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = PMAToUserBufferCopy
  [Called By]
  - >> DataStageOut
  - >> USB_SIL_Read

  SetCNTR (Thumb, 6 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetCNTR (Thumb, 8 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetISTR (Thumb, 8 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetISTR (Thumb, 10 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetFNR (Thumb, 10 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetDADDR (Thumb, 8 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetDADDR (Thumb, 10 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetBTABLE (Thumb, 14 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> Virtual_Com_Port_Reset

  GetBTABLE (Thumb, 10 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetENDPOINT (Thumb, 12 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetENDPOINT (Thumb, 16 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)
  [Called By]

  - >> SetDouBleBuffEPStall

  SetEPType (Thumb, 32 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPType
  [Called By]
  - >> Virtual_Com_Port_Reset

  GetEPType (Thumb, 18 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPTxStatus (Thumb, 60 bytes, Stack size 12 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetEPTxStatus
  [Called By]
  - >> Standard_ClearFeature
  - >> Virtual_Com_Port_Reset

  SetEPRxStatus (Thumb, 60 bytes, Stack size 12 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetEPRxStatus
  [Called By]
  - >> Virtual_Com_Port_Reset

  SetDouBleBuffEPStall (Thumb, 54 bytes, Stack size 12 bytes, usb_regs.o(.text), UNUSED)
  [Calls]

  - >> GetENDPOINT

  GetEPTxStatus (Thumb, 18 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetEPRxStatus (Thumb, 18 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPTxValid (Thumb, 48 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPTxValid
  [Called By]
  - >> EP1_IN_Callback

  SetEPRxValid (Thumb, 48 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPRxValid
  [Called By]
  - >> Virtual_Com_Port_Reset
  - >> EP3_OUT_Callback

  SetEP_KIND (Thumb, 38 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ClearEP_KIND (Thumb, 34 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  Clear_Status_Out (Thumb, 34 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> Virtual_Com_Port_Reset

  Set_Status_Out (Thumb, 38 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPDoubleBuff (Thumb, 38 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ClearEPDoubleBuff (Thumb, 34 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetTxStallStatus (Thumb, 28 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetRxStallStatus (Thumb, 30 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ClearEP_CTR_RX (Thumb, 32 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ClearEP_CTR_TX (Thumb, 28 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ToggleDTOG_RX (Thumb, 34 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ToggleDTOG_TX (Thumb, 34 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ClearDTOG_RX (Thumb, 48 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> Standard_ClearFeature

  ClearDTOG_TX (Thumb, 48 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> Standard_ClearFeature

  SetEPAddress (Thumb, 46 bytes, Stack size 8 bytes, usb_regs.o(.text), UNUSED)

  GetEPAddress (Thumb, 18 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPTxAddr (Thumb, 24 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPTxAddr
  [Called By]
  - >> Virtual_Com_Port_Reset

  SetEPRxAddr (Thumb, 26 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPRxAddr
  [Called By]
  - >> Virtual_Com_Port_Reset

  GetEPTxAddr (Thumb, 22 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> USB_SIL_Write
  - >> DataStageIn

  GetEPRxAddr (Thumb, 24 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> DataStageOut
  - >> USB_SIL_Read

  SetEPTxCount (Thumb, 20 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> USB_SIL_Write
  - >> DataStageIn
  - >> DataStageOut
  - >> EP1_IN_Callback

  SetEPCountRxReg (Thumb, 48 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPRxCount (Thumb, 68 bytes, Stack size 8 bytes, usb_regs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetEPRxCount
  [Called By]
  - >> Post0_Process
  - >> Standard_ClearFeature
  - >> Virtual_Com_Port_Reset

  GetEPTxCount (Thumb, 26 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetEPRxCount (Thumb, 26 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> USB_SIL_Read

  SetEPDblBuffAddr (Thumb, 44 bytes, Stack size 12 bytes, usb_regs.o(.text), UNUSED)

  SetEPDblBuf0Addr (Thumb, 24 bytes, Stack size 8 bytes, usb_regs.o(.text), UNUSED)

  SetEPDblBuf1Addr (Thumb, 26 bytes, Stack size 8 bytes, usb_regs.o(.text), UNUSED)

  GetEPDblBuf0Addr (Thumb, 22 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetEPDblBuf1Addr (Thumb, 24 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  SetEPDblBuffCount (Thumb, 186 bytes, Stack size 12 bytes, usb_regs.o(.text), UNUSED)

  SetEPDblBuf0Count (Thumb, 96 bytes, Stack size 12 bytes, usb_regs.o(.text), UNUSED)

  SetEPDblBuf1Count (Thumb, 96 bytes, Stack size 12 bytes, usb_regs.o(.text), UNUSED)

  GetEPDblBuf0Count (Thumb, 26 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetEPDblBuf1Count (Thumb, 26 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  GetEPDblBufDir (Thumb, 62 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  FreeUserBuffer (Thumb, 90 bytes, Stack size 8 bytes, usb_regs.o(.text), UNUSED)

  ToWord (Thumb, 8 bytes, Stack size 0 bytes, usb_regs.o(.text), UNUSED)

  ByteSwap (Thumb, 12 bytes, Stack size 0 bytes, usb_regs.o(.text))
  [Called By]

  - >> Setup0_Process

  USB_SIL_Init (Thumb, 28 bytes, Stack size 0 bytes, usb_sil.o(.text))
  [Called By]

  - >> Virtual_Com_Port_init

  USB_SIL_Write (Thumb, 46 bytes, Stack size 24 bytes, usb_sil.o(.text), UNUSED)
  [Calls]

  - >> GetEPTxAddr
  - >> UserToPMABufferCopy
  - >> SetEPTxCount

  USB_SIL_Read (Thumb, 46 bytes, Stack size 24 bytes, usb_sil.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = USB_SIL_Read ⇒ PMAToUserBufferCopy
  [Calls]
  - >> GetEPRxCount
  - >> PMAToUserBufferCopy
  - >> GetEPRxAddr
  [Called By]
  - >> EP3_OUT_Callback

  disk_status (Thumb, 28 bytes, Stack size 0 bytes, diskio.o(.text))
  [Called By]

  - >> validate
  - >> find_volume

  disk_initialize (Thumb, 42 bytes, Stack size 16 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = disk_initialize ⇒ SD_Init ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR
  [Calls]
  - >> SD_Init
  [Called By]
  - >> f_mkfs
  - >> find_volume

  disk_read (Thumb, 182 bytes, Stack size 552 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 648 + In Cycle
  - Call Chain = disk_read ⇒ disk_read (Cycle)
  [Calls]
  - >> SD_WaitReadOperation
  - >> SD_ReadMultiBlocks
  - >> SD_GetStatus
  - >> disk_read
  - >> __aeabi_memcpy
  [Called By]
  - >> f_write
  - >> f_lseek
  - >> f_read
  - >> move_window
  - >> disk_read

  disk_write (Thumb, 188 bytes, Stack size 552 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 648 + In Cycle
  - Call Chain = disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> SD_WriteMultiBlocks
  - >> SD_WaitWriteOperation
  - >> SD_GetStatus
  - >> disk_write
  - >> __aeabi_memcpy
  [Called By]
  - >> f_write
  - >> f_mkfs
  - >> f_truncate
  - >> f_lseek
  - >> f_sync
  - >> f_read
  - >> sync_fs
  - >> sync_window
  - >> disk_write

  disk_ioctl (Thumb, 102 bytes, Stack size 32 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = disk_ioctl ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> f_mkfs
  - >> find_volume
  - >> sync_fs

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, diskio.o(.text))
  [Called By]

  - >> f_open
  - >> f_mkfs
  - >> f_mkdir
  - >> f_sync

  clust2sect (Thumb, 26 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_write
  - >> f_rename
  - >> f_mkdir
  - >> f_lseek
  - >> f_read
  - >> dir_next
  - >> dir_sdi

  get_fat (Thumb, 318 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 728
  - Call Chain = get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> move_window
  [Called By]
  - >> f_truncate
  - >> f_getfree
  - >> f_lseek
  - >> f_read
  - >> dir_next
  - >> dir_sdi
  - >> create_chain
  - >> remove_chain

  put_fat (Thumb, 392 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 728
  - Call Chain = put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> move_window
  [Called By]
  - >> f_truncate
  - >> create_chain
  - >> remove_chain

  f_mount (Thumb, 86 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 832
  - Call Chain = f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> find_volume
  - >> get_ldnumber
  [Called By]
  - >> put_sd
  - >> get_sd_filename

  f_open (Thumb, 382 bytes, Stack size 600 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 1464
  - Call Chain = f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> find_volume
  - >> follow_path
  - >> dir_register
  - >> st_clust
  - >> ld_clust
  - >> remove_chain
  - >> move_window
  - >> get_fattime
  [Called By]
  - >> put_sd

  f_read (Thumb, 480 bytes, Stack size 72 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> mem_cpy
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> f_gets

  f_write (Thumb, 524 bytes, Stack size 64 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 824
  - Call Chain = f_write ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> clust2sect
  - >> validate
  - >> create_chain
  - >> mem_cpy
  - >> disk_write
  - >> disk_read
  [Called By]
  - >> put_sd
  - >> f_printf
  - >> f_puts
  - >> f_putc
  - >> putc_bfd

  f_sync (Thumb, 176 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 712
  - Call Chain = f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> validate
  - >> st_clust
  - >> sync_fs
  - >> move_window
  - >> get_fattime
  - >> disk_write
  [Called By]
  - >> f_close

  f_close (Thumb, 32 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 728
  - Call Chain = f_close ⇒ f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> f_sync
  - >> validate
  [Called By]
  - >> put_sd

  f_lseek (Thumb, 410 bytes, Stack size 32 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> clust2sect
  - >> validate
  - >> create_chain
  - >> disk_write
  - >> disk_read

  f_opendir (Thumb, 118 bytes, Stack size 552 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 1400
  - Call Chain = f_opendir ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> find_volume
  - >> follow_path
  - >> ld_clust
  - >> dir_sdi
  [Called By]
  - >> get_sd_filename

  f_closedir (Thumb, 22 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> validate

  f_readdir (Thumb, 100 bytes, Stack size 544 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 1368
  - Call Chain = f_readdir ⇒ dir_read ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> validate
  - >> get_fileinfo
  - >> dir_read
  - >> dir_next
  - >> dir_sdi
  [Called By]
  - >> get_sd_filename

  f_stat (Thumb, 68 bytes, Stack size 584 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> get_fileinfo

  f_getfree (Thumb, 258 bytes, Stack size 56 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat
  - >> find_volume
  - >> move_window

  f_truncate (Thumb, 184 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat
  - >> get_fat
  - >> validate
  - >> remove_chain
  - >> disk_write

  f_unlink (Thumb, 174 bytes, Stack size 616 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> dir_remove
  - >> dir_read
  - >> ld_clust
  - >> dir_sdi
  - >> remove_chain
  - >> sync_fs
  - >> mem_cpy

  f_mkdir (Thumb, 358 bytes, Stack size 600 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> find_volume
  - >> follow_path
  - >> dir_register
  - >> st_clust
  - >> create_chain
  - >> remove_chain
  - >> sync_fs
  - >> sync_window
  - >> mem_set
  - >> mem_cpy
  - >> get_fattime

  f_chmod (Thumb, 92 bytes, Stack size 592 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> sync_fs

  f_rename (Thumb, 266 bytes, Stack size 648 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect
  - >> find_volume
  - >> get_ldnumber
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> st_clust
  - >> ld_clust
  - >> sync_fs
  - >> move_window
  - >> mem_cpy

  f_utime (Thumb, 94 bytes, Stack size 584 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> find_volume
  - >> follow_path
  - >> sync_fs

  f_mkfs (Thumb, 1622 bytes, Stack size 112 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_ldnumber
  - >> mem_set
  - >> mem_cpy
  - >> get_fattime
  - >> disk_ioctl
  - >> disk_write
  - >> disk_initialize

  f_gets (Thumb, 82 bytes, Stack size 40 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_read

  f_putc (Thumb, 64 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_write
  - >> putc_bfd

  f_puts (Thumb, 74 bytes, Stack size 96 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_write
  - >> putc_bfd

  f_printf (Thumb, 674 bytes, Stack size 160 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_write
  - >> putc_bfd

  ff_convert (Thumb, 116 bytes, Stack size 24 bytes, cc936.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = ff_convert
  [Called By]
  - >> create_name
  - >> get_fileinfo

  ff_wtoupper (Thumb, 84 bytes, Stack size 12 bytes, cc936.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ff_wtoupper
  [Called By]
  - >> create_name
  - >> cmp_lfn

  SD_DeInit (Thumb, 66 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SetPowerState
  - >> SDIO_ClockCmd
  - >> SDIO_DeInit
  - >> GPIO_Init
  - >> RCC_AHBPeriphClockCmd

  SD_EnableWideBusOperation (Thumb, 140 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR
  [Calls]
  - >> SDIO_Init
  - >> SDEnWideBus
  [Called By]
  - >> SD_Init

  SD_SelectDeselect (Thumb, 48 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_SelectDeselect
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_GetCardInfo (Thumb, 764 bytes, Stack size 20 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SD_GetCardInfo
  [Called By]
  - >> SD_Init

  SD_InitializeCards (Thumb, 294 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = SD_InitializeCards ⇒ CmdResp6Error ⇒ SDIO_GetResponse
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_SendCommand
  - >> SDIO_GetPowerState
  - >> CmdResp6Error
  - >> CmdResp2Error
  [Called By]
  - >> SD_Init

  SD_PowerON (Thumb, 374 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_PowerON ⇒ CmdError
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_SendCommand
  - >> SDIO_SetPowerState
  - >> SDIO_ClockCmd
  - >> SDIO_Init
  - >> CmdError
  - >> CmdResp7Error
  - >> CmdResp3Error
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_Init (Thumb, 138 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = SD_Init ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR
  [Calls]
  - >> SDIO_Init
  - >> SDIO_DeInit
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_GetCardInfo
  - >> SD_SelectDeselect
  - >> SD_EnableWideBusOperation
  - >> GPIO_Configuration
  - >> NVIC_Configuration
  [Called By]
  - >> disk_initialize

  SD_SendStatus (Thumb, 46 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_SendStatus
  [Calls]
  - >> CmdResp1Error
  [Called By]
  - >> SD_GetState

  SD_GetState (Thumb, 26 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_GetState ⇒ SD_SendStatus
  [Calls]
  - >> SD_SendStatus
  [Called By]
  - >> SD_GetStatus

  SD_GetStatus (Thumb, 30 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SD_GetStatus ⇒ SD_GetState ⇒ SD_SendStatus
  [Calls]
  - >> SD_GetState
  [Called By]
  - >> disk_write
  - >> disk_read

  SD_PowerOFF (Thumb, 14 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SetPowerState

  SD_SendSDStatus (Thumb, 360 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_ClearFlag
  - >> SDIO_GetFlagStatus
  - >> SDIO_ReadData
  - >> SDIO_DataConfig
  - >> SDIO_GetResponse
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_GetCardStatus

  SD_GetCardStatus (Thumb, 156 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SD_SendSDStatus

  SD_ReadBlock (Thumb, 208 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_DataConfig
  - >> SDIO_SendCommand
  - >> SDIO_DMACmd
  - >> SDIO_ITConfig
  - >> CmdResp1Error
  - >> SD_DMA_RxConfig
  - >> __aeabi_uldivmod

  SD_ReadMultiBlocks (Thumb, 264 bytes, Stack size 32 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = SD_ReadMultiBlocks ⇒ SD_DMA_RxConfig ⇒ DMA_Init
  [Calls]
  - >> SDIO_DataConfig
  - >> SDIO_SendCommand
  - >> SDIO_DMACmd
  - >> SDIO_ITConfig
  - >> CmdResp1Error
  - >> SD_DMA_RxConfig
  - >> __aeabi_uldivmod
  [Called By]
  - >> disk_read

  SD_WaitReadOperation (Thumb, 42 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_WaitReadOperation ⇒ SD_DMAEndOfTransferStatus
  [Calls]
  - >> SD_DMAEndOfTransferStatus
  [Called By]
  - >> disk_read

  SD_WriteBlock (Thumb, 206 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_DataConfig
  - >> SDIO_SendCommand
  - >> SDIO_DMACmd
  - >> SDIO_ITConfig
  - >> CmdResp1Error
  - >> SD_DMA_TxConfig
  - >> __aeabi_uldivmod

  SD_WriteMultiBlocks (Thumb, 312 bytes, Stack size 32 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = SD_WriteMultiBlocks ⇒ SD_DMA_TxConfig ⇒ DMA_Init
  [Calls]
  - >> SDIO_DataConfig
  - >> SDIO_SendCommand
  - >> SDIO_DMACmd
  - >> SDIO_ITConfig
  - >> CmdResp1Error
  - >> SD_DMA_TxConfig
  - >> __aeabi_uldivmod
  [Called By]
  - >> disk_write

  SD_WaitWriteOperation (Thumb, 50 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SD_WaitWriteOperation ⇒ SD_DMAEndOfTransferStatus
  [Calls]
  - >> SDIO_ClearFlag
  - >> SD_DMAEndOfTransferStatus
  [Called By]
  - >> disk_write

  SD_GetTransferState (Thumb, 18 bytes, Stack size 0 bytes, bsp_sdio_sdcard.o(.text), UNUSED)

  SD_StopTransfer (Thumb, 28 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> CmdResp1Error

  SD_Erase (Thumb, 290 bytes, Stack size 32 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_GetResponse
  - >> SDIO_SendCommand
  - >> IsCardProgramming
  - >> CmdResp1Error

  SD_ProcessIRQSrc (Thumb, 70 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_ProcessIRQSrc
  [Calls]
  - >> SDIO_ClearITPendingBit
  - >> SDIO_ITConfig
  - >> CmdResp1Error
  [Called By]
  - >> SDIO_IRQHandler

  convert_from_bytes_to_power_of_two (Thumb, 18 bytes, Stack size 0 bytes, bsp_sdio_sdcard.o(.text), UNUSED)

  WIZ_RCC_PLLConfig (Thumb, 28 bytes, Stack size 24 bytes, w55mh32.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = WIZ_RCC_PLLConfig ⇒ MH_RCC_PLLConfig
  [Calls]
  - >> MH_RCC_PLLConfig
  [Called By]
  - >> rcc_clk_config

  WIZ_LSE_DriveConfig (Thumb, 20 bytes, Stack size 16 bytes, w55mh32.o(.text), UNUSED)
  [Calls]

  - >> MH_LSE_DriveConfig

  WIZ_PLL_SelLockConfig (Thumb, 20 bytes, Stack size 16 bytes, w55mh32.o(.text), UNUSED)
  [Calls]

  - >> MH_PLL_SelLockConfig

  WIZ_PLL_CpConfig (Thumb, 20 bytes, Stack size 16 bytes, w55mh32.o(.text), UNUSED)
  [Calls]

  - >> MH_PLL_CpConfig

  MH_RCC_PLLConfig (Thumb, 236 bytes, Stack size 32 bytes, mh.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MH_RCC_PLLConfig
  [Called By]
  - >> WIZ_RCC_PLLConfig

  MH_LSE_DriveConfig (Thumb, 74 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)
  [Called By]

  - >> WIZ_LSE_DriveConfig

  MH_PLL_SelLockConfig (Thumb, 128 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)
  [Called By]

  - >> WIZ_PLL_SelLockConfig

  MH_PLL_CpConfig (Thumb, 96 bytes, Stack size 0 bytes, mh.o(.text), UNUSED)
  [Called By]

  - >> WIZ_PLL_CpConfig

  MH_FLASH_FastProgramPage (Thumb, 374 bytes, Stack size 56 bytes, mh.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks
  - >> disk_ioctl
  - >> _printf_core
  - >> _fp_digits

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> check_eeprom_network_info
  - >> send_http_response_header
  - >> disk_write
  - >> disk_read

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> send_http_response_body
  - >> predefined_get_cgi_processor
  - >> make_json_update_page

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> check_eeprom_network_info
  - >> http_process_handler
  - >> predefined_get_cgi_processor
  - >> make_json_update_page

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strcat (Thumb, 24 bytes, Stack size 0 bytes, strcat.o(.text))
  [Called By]

  - >> make_http_response_head
  - >> predefined_get_cgi_processor
  - >> make_json_update_page

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> mid
  - >> find_http_uri_type
  - >> get_http_param_value

  strncpy (Thumb, 24 bytes, Stack size 8 bytes, strncpy.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strncpy
  [Called By]
  - >> usb_run
  - >> read_userReg_webContent
  - >> mid
  - >> get_http_param_value

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> reg_httpServer_webContent
  - >> read_userReg_webContent
  - >> send_http_response_header
  - >> mid
  - >> usb_printf
  - >> get_http_param_value

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> http_post_cgi_handler
  - >> http_get_cgi_handler
  - >> find_userReg_webContent
  - >> http_process_handler
  - >> get_http_uri_name
  - >> parse_http_request
  - >> get_sd_filename
  - >> predefined_set_cgi_processor
  - >> predefined_get_cgi_processor

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> reg_httpServer_webContent
  - >> http_process_handler
  - >> send_http_response_body
  - >> inet_addr_
  - >> get_http_uri_name
  - >> parse_http_request
  - >> make_http_response_head
  - >> get_sd_filename
  - >> predefined_set_cgi_processor
  - >> set_netinfo

  strtok (Thumb, 62 bytes, Stack size 16 bytes, strtok.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = strtok
  [Called By]
  - >> inet_addr_
  - >> get_http_uri_name
  - >> parse_http_request

  __0sscanf (Thumb, 48 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> parse_ip

  _scanf_int (Thumb, 332 bytes, Stack size 56 bytes, _scanf_int.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_int
  [Calls]
  - >> _chval
  [Called By]
  - >> __vfscanf

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> __aeabi_fsub
  - >> __aeabi_frsub

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> MYI2C_Handle

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fadd

  __aeabi_fmul (Thumb, 100 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> MYI2C_Handle

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> MYI2C_Handle

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> MYI2C_Handle

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> make_json_update_page

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_int

  __vfscanf_char (Thumb, 20 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv
  - >> __aeabi_fadd

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f
  - >> __aeabi_fadd

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> _double_round
  - >> _double_epilogue
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  isspace (Thumb, 10 bytes, Stack size 0 bytes, isspace_c.o(.text))
  [Calls]

  - >> __ctype_lookup
  [Address Reference Count : 1]
  - scanf_char.o(.text)

  __vfscanf (Thumb, 810 bytes, Stack size 88 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _scanf_int
  [Called By]
  - >> __vfscanf_char

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text), UNUSED)
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __ctype_lookup (Thumb, 34 bytes, Stack size 0 bytes, ctype_c.o(.text))
  [Called By]

  - >> isspace

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  WIZCHIP_READ (Thumb, 98 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.WIZCHIP_READ))
  [Stack]

  - Max Depth = 24
  - Call Chain = WIZCHIP_READ
  [Called By]
  - >> wiz_toe_init
  - >> httpServer_run
  - >> http_disconnect
  - >> check_DHCP_leasedIP
  - >> default_ip_conflict
  - >> default_ip_update
  - >> wizphy_getphystat
  - >> wizchip_setnetmode
  - >> wizchip_getnetmode
  - >> wizchip_gettimeout
  - >> wizchip_sw_reset
  - >> wizchip_getinterrupt
  - >> wizchip_getinterruptmask
  - >> wizphy_getphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> wizphy_getphypmode
  - >> wizphy_getphylink
  - >> wiz_send_data
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> getSn_TX_FSR
  - >> getSn_RX_RSR
  - >> getsockopt
  - >> setsockopt
  - >> ctlsocket
  - >> recvfrom
  - >> sendto
  - >> recv
  - >> send
  - >> disconnect
  - >> connect
  - >> listen
  - >> socket
  - >> close
  - >> ctlwizchip
  - >> DHCP_run
  - >> wiz_print_phy_info

  WIZCHIP_READ_BUF (Thumb, 120 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.WIZCHIP_READ_BUF))
  [Stack]

  - Max Depth = 24
  - Call Chain = WIZCHIP_READ_BUF
  [Called By]
  - >> wizchip_getnetinfo
  - >> httpServer_run
  - >> makeDHCPMSG
  - >> wizchip_sw_reset
  - >> wiz_recv_data
  - >> getsockopt
  - >> socket
  - >> DHCP_init
  - >> wiz_dhcp_process

  WIZCHIP_WRITE (Thumb, 100 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.WIZCHIP_WRITE))
  [Stack]

  - Max Depth = 24
  - Call Chain = WIZCHIP_WRITE
  [Called By]
  - >> httpServer_run
  - >> http_disconnect
  - >> check_DHCP_leasedIP
  - >> default_ip_conflict
  - >> default_ip_update
  - >> wizchip_setnetmode
  - >> wizchip_settimeout
  - >> wizchip_init
  - >> wizchip_sw_reset
  - >> wizchip_clrinterrupt
  - >> wizchip_setinterruptmask
  - >> wizphy_setphyconf
  - >> wizphy_setphypmode
  - >> wizphy_reset
  - >> wiz_send_data
  - >> wiz_recv_ignore
  - >> wiz_recv_data
  - >> setsockopt
  - >> ctlsocket
  - >> recvfrom
  - >> sendto
  - >> recv
  - >> send
  - >> disconnect
  - >> connect
  - >> listen
  - >> socket
  - >> close
  - >> ctlwizchip

  WIZCHIP_WRITE_BUF (Thumb, 126 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text.WIZCHIP_WRITE_BUF))
  [Stack]

  - Max Depth = 32
  - Call Chain = WIZCHIP_WRITE_BUF
  [Called By]
  - >> default_ip_conflict
  - >> default_ip_update
  - >> default_ip_assign
  - >> wizchip_sw_reset
  - >> wiz_send_data
  - >> setsockopt
  - >> sendto
  - >> connect
  - >> wizchip_setnetinfo
  - >> DHCP_init

  getSn_RX_RSR (Thumb, 76 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.getSn_RX_RSR))
  [Stack]

  - Max Depth = 48
  - Call Chain = getSn_RX_RSR ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run
  - >> parseDHCPMSG
  - >> getsockopt
  - >> recvfrom
  - >> recv

  getSn_TX_FSR (Thumb, 76 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.getSn_TX_FSR))
  [Stack]

  - Max Depth = 48
  - Call Chain = getSn_TX_FSR ⇒ WIZCHIP_READ
  [Calls]
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run
  - >> getsockopt
  - >> sendto
  - >> recv
  - >> send

  wiz_recv_data (Thumb, 100 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text.wiz_recv_data))
  [Stack]

  - Max Depth = 56
  - Call Chain = wiz_recv_data ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ_BUF
  - >> WIZCHIP_READ
  [Called By]
  - >> recvfrom
  - >> recv

  wiz_recv_ignore (Thumb, 66 bytes, Stack size 24 bytes, w55mh32_wztoe.o(.text.wiz_recv_ignore))
  [Stack]

  - Max Depth = 48
  - Call Chain = wiz_recv_ignore ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> recvfrom

  wiz_send_data (Thumb, 100 bytes, Stack size 32 bytes, w55mh32_wztoe.o(.text.wiz_send_data))
  [Stack]

  - Max Depth = 64
  - Call Chain = wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> WIZCHIP_WRITE_BUF
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> sendto
  - >> send

  wiz_toe_init (Thumb, 92 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text.wiz_toe_init))
  [Stack]

  - Max Depth = 96
  - Call Chain = wiz_toe_init ⇒ wiztoe_bus_init ⇒ GPIO_Init
  [Calls]
  - >> reg_wizchip_spiburst_cbfunc
  - >> reg_wizchip_spi_cbfunc
  - >> reg_wizchip_cs_cbfunc
  - >> WIZCHIP_READ
  - >> wiztoe_hw_reset
  - >> wiztoe_delay
  - >> wiztoe_bus_init
  [Called By]
  - >> main

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> wiz_phy_link_check
  - >> usb_run
  - >> httpServer_run
  - >> check_eeprom_network_info
  - >> main
  - >> display_reg_webContent_list
  - >> http_process_handler
  - >> send_http_response_cgi
  - >> send_http_response_header
  - >> send_http_response_body
  - >> put_sd
  - >> get_sd_filename
  - >> predefined_get_cgi_processor
  - >> make_json_update_page
  - >> ee_Erase
  - >> print_network_information
  - >> wiz_print_phy_info
  - >> wiz_dhcp_process
  - >> USART_Config
  - >> USB_Cable_Config
  - >> Leave_LowPowerMode
  - >> Enter_LowPowerMode

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> http_post_cgi_handler
  - >> send_http_response_cgi
  - >> make_http_response_head
  - >> predefined_set_cgi_processor
  - >> set_netinfo
  - >> predefined_get_cgi_processor
  - >> make_json_netinfo
  - >> make_json_update_page

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __0vsprintf (Thumb, 30 bytes, Stack size 24 bytes, printfa.o(i.__0vsprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1vsprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0vsprintf), UNUSED)

  __2vsprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0vsprintf), UNUSED)

  __c89vsprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0vsprintf), UNUSED)

  vsprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0vsprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = vsprintf
  [Called By]
  - >> usb_printf

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> reg_httpServer_webContent

  ### Local Symbols

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 108 bytes, Stack size 20 bytes, w55mh32_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_w55mh32.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  wiz_dhcp_process (Thumb, 146 bytes, Stack size 48 bytes, wiz_interface.o(.text))
  [Stack]

  - Max Depth = 208
  - Call Chain = wiz_dhcp_process ⇒ DHCP_run ⇒ check_DHCP_leasedIP ⇒ send_DHCP_DECLINE ⇒ sendto ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> wizchip_setnetinfo
  - >> getSNfromDHCP
  - >> getIPfromDHCP
  - >> getGWfromDHCP
  - >> getDNSfromDHCP
  - >> WIZCHIP_READ_BUF
  - >> DHCP_stop
  - >> DHCP_run
  - >> DHCP_init
  - >> __2printf
  [Called By]
  - >> network_init

  i2c_Delay (Thumb, 10 bytes, Stack size 8 bytes, eeprom.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = i2c_Delay
  [Calls]
  - >> delay_us
  [Called By]
  - >> i2c_NAck
  - >> i2c_Ack
  - >> i2c_WaitAck
  - >> i2c_ReadByte
  - >> i2c_SendByte
  - >> i2c_Start
  - >> i2c_Stop

  parse_ip (Thumb, 50 bytes, Stack size 40 bytes, userhandler.o(.text))
  [Stack]

  - Max Depth = 256
  - Call Chain = parse_ip ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __0sscanf
  [Called By]
  - >> set_netinfo

  C2D (Thumb, 54 bytes, Stack size 0 bytes, httpparser.o(.text))
  [Called By]

  - >> unescape_http_url
  - >> ATOI

  replacetochar (Thumb, 26 bytes, Stack size 8 bytes, httpparser.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = replacetochar
  [Called By]
  - >> get_http_param_value

  getHTTPSocketNum (Thumb, 8 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Called By]

  - >> httpServer_run

  getHTTPSequenceNum (Thumb, 32 bytes, Stack size 0 bytes, httpserver.o(.text))
  [Called By]

  - >> http_process_handler
  - >> send_http_response_body

  http_disconnect (Thumb, 48 bytes, Stack size 8 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = http_disconnect ⇒ WIZCHIP_WRITE
  [Calls]
  - >> WIZCHIP_WRITE
  - >> WIZCHIP_READ
  [Called By]
  - >> httpServer_run

  send_http_response_body (Thumb, 530 bytes, Stack size 40 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = send_http_response_body ⇒ send ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> read_userReg_webContent
  - >> getHTTPSequenceNum
  - >> send
  - >> __2printf
  - >> strcpy
  - >> __aeabi_memclr
  [Called By]
  - >> httpServer_run
  - >> http_process_handler

  send_http_response_header (Thumb, 172 bytes, Stack size 24 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = send_http_response_header ⇒ send ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> make_http_response_head
  - >> send
  - >> __2printf
  - >> strlen
  - >> __aeabi_memcpy
  [Called By]
  - >> http_process_handler

  send_http_response_cgi (Thumb, 922 bytes, Stack size 32 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = send_http_response_cgi ⇒ send ⇒ wiz_send_data ⇒ WIZCHIP_WRITE_BUF
  [Calls]
  - >> send
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> http_process_handler

  http_process_handler (Thumb, 620 bytes, Stack size 1512 bytes, httpserver.o(.text))
  [Stack]

  - Max Depth = 11640
  - Call Chain = http_process_handler ⇒ http_post_cgi_handler ⇒ predefined_set_cgi_processor ⇒ put_sd ⇒ f_open ⇒ dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> http_post_cgi_handler
  - >> http_get_cgi_handler
  - >> find_userReg_webContent
  - >> send_http_response_cgi
  - >> send_http_response_header
  - >> send_http_response_body
  - >> getHTTPSequenceNum
  - >> get_http_uri_name
  - >> mid
  - >> find_http_uri_type
  - >> __2printf
  - >> strcpy
  - >> strcmp
  - >> __aeabi_memclr4
  [Called By]
  - >> httpServer_run

  DataStageOut (Thumb, 166 bytes, Stack size 24 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = DataStageOut ⇒ PMAToUserBufferCopy
  [Calls]
  - >> PMAToUserBufferCopy
  - >> GetEPRxAddr
  - >> SetEPTxCount
  [Called By]
  - >> Out0_Process

  DataStageIn (Thumb, 166 bytes, Stack size 32 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> GetEPTxAddr
  - >> UserToPMABufferCopy
  - >> SetEPTxCount
  [Called By]
  - >> In0_Process
  - >> Data_Setup0

  NoData_Setup0 (Thumb, 290 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = NoData_Setup0 ⇒ Standard_ClearFeature ⇒ SetEPTxStatus
  [Calls]
  - >> Standard_SetDeviceFeature
  - >> Standard_SetEndPointFeature
  - >> Standard_ClearFeature
  - >> Standard_SetInterface
  - >> Standard_SetConfiguration
  [Called By]
  - >> Setup0_Process

  Data_Setup0 (Thumb, 678 bytes, Stack size 40 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = Data_Setup0 ⇒ DataStageIn ⇒ UserToPMABufferCopy
  [Calls]
  - >> DataStageIn
  [Called By]
  - >> Setup0_Process

  mem_cpy (Thumb, 26 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = mem_cpy
  [Called By]
  - >> f_write
  - >> f_mkfs
  - >> f_rename
  - >> f_mkdir
  - >> f_unlink
  - >> f_read
  - >> dir_register
  - >> gen_numname

  mem_set (Thumb, 20 bytes, Stack size 12 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = mem_set
  [Called By]
  - >> f_mkfs
  - >> f_mkdir
  - >> create_name
  - >> dir_remove
  - >> dir_register
  - >> dir_next
  - >> sync_fs

  mem_cmp (Thumb, 38 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = mem_cmp
  [Called By]
  - >> dir_find

  chk_chr (Thumb, 20 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> create_name

  sync_window (Thumb, 82 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 672
  - Call Chain = sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> disk_write
  [Called By]
  - >> f_mkdir
  - >> dir_next
  - >> sync_fs
  - >> move_window

  move_window (Thumb, 52 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 688
  - Call Chain = move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> sync_window
  - >> disk_read
  [Called By]
  - >> f_open
  - >> f_rename
  - >> f_getfree
  - >> f_sync
  - >> put_fat
  - >> get_fat
  - >> find_volume
  - >> check_fs
  - >> dir_remove
  - >> dir_register
  - >> dir_read
  - >> dir_find
  - >> dir_alloc

  sync_fs (Thumb, 200 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 688
  - Call Chain = sync_fs ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> sync_window
  - >> mem_set
  - >> disk_ioctl
  - >> disk_write
  [Called By]
  - >> f_utime
  - >> f_rename
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink
  - >> f_sync

  remove_chain (Thumb, 108 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 752
  - Call Chain = remove_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_open
  - >> f_mkdir
  - >> f_unlink
  - >> f_truncate

  create_chain (Thumb, 214 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 760
  - Call Chain = create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_write
  - >> f_mkdir
  - >> f_lseek
  - >> dir_next

  dir_sdi (Thumb, 200 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 752
  - Call Chain = dir_sdi ⇒ get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> get_fat
  - >> clust2sect
  [Called By]
  - >> f_readdir
  - >> f_opendir
  - >> f_unlink
  - >> follow_path
  - >> dir_remove
  - >> dir_register
  - >> dir_find
  - >> dir_alloc

  dir_next (Thumb, 314 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 784
  - Call Chain = dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> get_fat
  - >> clust2sect
  - >> create_chain
  - >> sync_window
  - >> mem_set
  [Called By]
  - >> f_readdir
  - >> dir_remove
  - >> dir_register
  - >> dir_read
  - >> dir_find
  - >> dir_alloc

  dir_alloc (Thumb, 92 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 808
  - Call Chain = dir_alloc ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> dir_next
  - >> dir_sdi
  - >> move_window
  [Called By]
  - >> dir_register

  ld_clust (Thumb, 32 bytes, Stack size 8 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ld_clust
  [Called By]
  - >> f_opendir
  - >> f_open
  - >> f_rename
  - >> f_unlink
  - >> follow_path

  st_clust (Thumb, 16 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_open
  - >> f_rename
  - >> f_mkdir
  - >> f_sync

  cmp_lfn (Thumb, 154 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = cmp_lfn ⇒ ff_wtoupper
  [Calls]
  - >> ff_wtoupper
  [Called By]
  - >> dir_find

  pick_lfn (Thumb, 124 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = pick_lfn
  [Called By]
  - >> dir_read

  fit_lfn (Thumb, 122 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = fit_lfn
  [Called By]
  - >> dir_register

  gen_numname (Thumb, 198 bytes, Stack size 64 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = gen_numname ⇒ mem_cpy
  [Calls]
  - >> mem_cpy
  [Called By]
  - >> dir_register

  sum_sfn (Thumb, 32 bytes, Stack size 12 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = sum_sfn
  [Called By]
  - >> dir_register
  - >> dir_read
  - >> dir_find

  dir_find (Thumb, 234 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 816
  - Call Chain = dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> sum_sfn
  - >> cmp_lfn
  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_cmp
  [Called By]
  - >> follow_path
  - >> dir_register

  dir_read (Thumb, 206 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 824
  - Call Chain = dir_read ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> sum_sfn
  - >> pick_lfn
  - >> dir_next
  - >> move_window
  [Called By]
  - >> f_readdir
  - >> f_unlink

  dir_register (Thumb, 298 bytes, Stack size 48 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 864
  - Call Chain = dir_register ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> dir_find
  - >> sum_sfn
  - >> gen_numname
  - >> fit_lfn
  - >> dir_alloc
  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_set
  - >> mem_cpy
  [Called By]
  - >> f_open
  - >> f_rename
  - >> f_mkdir

  dir_remove (Thumb, 106 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> dir_next
  - >> dir_sdi
  - >> move_window
  - >> mem_set
  [Called By]
  - >> f_rename
  - >> f_unlink

  get_fileinfo (Thumb, 272 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = get_fileinfo ⇒ ff_convert
  [Calls]
  - >> ff_convert
  [Called By]
  - >> f_readdir
  - >> f_stat

  create_name (Thumb, 604 bytes, Stack size 56 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = create_name ⇒ ff_convert
  [Calls]
  - >> ff_wtoupper
  - >> ff_convert
  - >> chk_chr
  - >> mem_set
  [Called By]
  - >> follow_path

  follow_path (Thumb, 144 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 848
  - Call Chain = follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> create_name
  - >> dir_find
  - >> ld_clust
  - >> dir_sdi
  [Called By]
  - >> f_opendir
  - >> f_open
  - >> f_utime
  - >> f_rename
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink
  - >> f_stat

  get_ldnumber (Thumb, 74 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = get_ldnumber
  [Called By]
  - >> f_mount
  - >> f_mkfs
  - >> f_rename
  - >> find_volume

  check_fs (Thumb, 140 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 704
  - Call Chain = check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> move_window
  [Called By]
  - >> find_volume

  find_volume (Thumb, 996 bytes, Stack size 88 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 792
  - Call Chain = find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write ⇒ disk_write (Cycle)
  [Calls]
  - >> check_fs
  - >> get_ldnumber
  - >> move_window
  - >> disk_ioctl
  - >> disk_initialize
  - >> disk_status
  [Called By]
  - >> f_opendir
  - >> f_open
  - >> f_mount
  - >> f_utime
  - >> f_rename
  - >> f_chmod
  - >> f_mkdir
  - >> f_unlink
  - >> f_getfree
  - >> f_stat

  validate (Thumb, 50 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = validate
  [Calls]
  - >> disk_status
  [Called By]
  - >> f_write
  - >> f_readdir
  - >> f_close
  - >> f_truncate
  - >> f_closedir
  - >> f_lseek
  - >> f_sync
  - >> f_read

  putc_bfd (Thumb, 68 bytes, Stack size 24 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> f_write
  [Called By]
  - >> f_printf
  - >> f_puts
  - >> f_putc

  NVIC_Configuration (Thumb, 40 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = NVIC_Configuration ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> SD_Init

  SD_DMAEndOfTransferStatus (Thumb, 10 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SD_DMAEndOfTransferStatus
  [Calls]
  - >> DMA_GetFlagStatus
  [Called By]
  - >> SD_WaitWriteOperation
  - >> SD_WaitReadOperation

  SD_DMA_RxConfig (Thumb, 86 bytes, Stack size 56 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = SD_DMA_RxConfig ⇒ DMA_Init
  [Calls]
  - >> DMA_ClearFlag
  - >> DMA_Cmd
  - >> DMA_Init
  [Called By]
  - >> SD_ReadBlock
  - >> SD_ReadMultiBlocks

  SD_DMA_TxConfig (Thumb, 86 bytes, Stack size 56 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = SD_DMA_TxConfig ⇒ DMA_Init
  [Calls]
  - >> DMA_ClearFlag
  - >> DMA_Cmd
  - >> DMA_Init
  [Called By]
  - >> SD_WriteBlock
  - >> SD_WriteMultiBlocks

  GPIO_Configuration (Thumb, 70 bytes, Stack size 8 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  [Called By]
  - >> SD_Init

  CmdResp1Error (Thumb, 40 bytes, Stack size 0 bytes, bsp_sdio_sdcard.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_Erase
  - >> SD_StopTransfer
  - >> SD_WriteBlock
  - >> SD_ReadBlock
  - >> SD_SendSDStatus
  - >> SD_SendStatus
  - >> SD_PowerON
  - >> SD_SelectDeselect
  - >> SDEnWideBus
  - >> FindSCR
  - >> SD_WriteMultiBlocks
  - >> SD_ReadMultiBlocks

  FindSCR (Thumb, 396 bytes, Stack size 32 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = FindSCR
  [Calls]
  - >> SDIO_ClearFlag
  - >> SDIO_GetFlagStatus
  - >> SDIO_ReadData
  - >> SDIO_DataConfig
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SDEnWideBus

  SDEnWideBus (Thumb, 310 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SDEnWideBus ⇒ FindSCR
  [Calls]
  - >> SDIO_GetResponse
  - >> SDIO_SendCommand
  - >> FindSCR
  - >> CmdResp1Error
  [Called By]
  - >> SD_EnableWideBusOperation

  CmdResp2Error (Thumb, 100 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp2Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  CmdResp6Error (Thumb, 152 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CmdResp6Error ⇒ SDIO_GetResponse
  [Calls]
  - >> SDIO_ClearFlag
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  [Called By]
  - >> SD_InitializeCards

  CmdResp3Error (Thumb, 52 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp3Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_PowerON

  CmdResp7Error (Thumb, 72 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp7Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_PowerON

  CmdError (Thumb, 44 bytes, Stack size 16 bytes, bsp_sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdError
  [Calls]
  - >> SDIO_ClearFlag
  - >> SDIO_GetFlagStatus
  [Called By]
  - >> SD_PowerON

  IsCardProgramming (Thumb, 434 bytes, Stack size 24 bytes, bsp_sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_ClearFlag
  - >> SDIO_GetResponse
  - >> SDIO_GetCommandResponse
  - >> SDIO_SendCommand
  [Called By]
  - >> SD_Erase

  wiz_deselect (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text.wiz_deselect), UNUSED)
  [Calls]

  - >> GPIO_SetBits

  wiz_read_buff (Thumb, 26 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text.wiz_read_buff), UNUSED)
  [Calls]

  - >> wiz_read_byte

  wiz_read_byte (Thumb, 54 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text.wiz_read_byte), UNUSED)
  [Calls]

  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_SendData
  [Called By]
  - >> wiz_read_buff

  wiz_select (Thumb, 20 bytes, Stack size 8 bytes, w55mh32_wztoe.o(.text.wiz_select), UNUSED)
  [Calls]

  - >> GPIO_ResetBits

  wiz_write_buff (Thumb, 26 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text.wiz_write_buff), UNUSED)
  [Calls]

  - >> wiz_write_byte

  wiz_write_byte (Thumb, 52 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text.wiz_write_byte), UNUSED)
  [Calls]

  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_SendData
  [Called By]
  - >> wiz_write_buff

  wiztoe_bus_init (Thumb, 180 bytes, Stack size 64 bytes, w55mh32_wztoe.o(.text.wiztoe_bus_init))
  [Stack]

  - Max Depth = 88
  - Call Chain = wiztoe_bus_init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Cmd
  - >> SPI_Init
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_GetClocksFreq
  [Called By]
  - >> wiz_toe_init

  wiztoe_delay (Thumb, 30 bytes, Stack size 4 bytes, w55mh32_wztoe.o(.text.wiztoe_delay))
  [Stack]

  - Max Depth = 4
  - Call Chain = wiztoe_delay
  [Called By]
  - >> wiz_toe_init
  - >> wiztoe_hw_reset

  wiztoe_hw_reset (Thumb, 84 bytes, Stack size 16 bytes, w55mh32_wztoe.o(.text.wiztoe_hw_reset))
  [Stack]

  - Max Depth = 40
  - Call Chain = wiztoe_hw_reset ⇒ GPIO_Init
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> wiztoe_delay
  [Called By]
  - >> wiz_toe_init

  _fp_digits (Thumb, 366 bytes, Stack size 64 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  - >> __aeabi_uldivmod
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1704 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  - >> __aeabi_uldivmod
  [Called By]
  - >> __0vsprintf
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0vsprintf
  - >> __0sprintf
  [Address Reference Count : 2]
  - printfa.o(i.__0sprintf)
  - printfa.o(i.__0vsprintf)

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  ### Undefined Global Symbols